J 	J	!:.. 	jyj

RB-35PW-OED3

-----------.

SPECIFICATIONS OF 	GEARED MOTOR

1 SCOPE
THE SPECIFICATIONS COVERS GEARED MOTORS RB-35PM-OED3 TO BE SUPPLIED
BY SAYAKA SEIIHTU KOGYO.

2 	TYPE  AND 	NAME

2-1 Geared motor
2-2 Motor
2-3 Gear head
2-4 Reduction ratio

:Type RB-35PM-OED3
:Type SK35-T06-U1
:Type RB-35P-OED3
:1/100

3 	SPECIFICATIONS FOR 	APPEARANCE

3-1 External dimensions
3-2 Appearance
3-3 Output shaft Radial play

3-4 Output shaft Thrust play

:As per separate external drawings.
:No flaw or damage shall be observed.
:Max 0. 1  mm  (A load of 113g   perpendicular to the shaft
at a point 3mm from the end of the bearing)
:Yax 0. 35mm

4 	ELECTRICAL	PROPERTIES
These show characteristics at a room temperature and normal humidity,
but may vary according to the actual values obtainable at mass-production

4 - 1 Rated voltage
4 - 2  Rated allowable torque
4 - 3  Rated speed
4 - 4  Rated current
4 - 5  No load speed
4 - 6  No load current
4 - 7 Insulation resistance

4- 8 Dielectric strength

:DC12V
:3. 3kg • em
:52±8. 8rpm
:390mA MAX
:59± 8. 9rpm
:120mA  MAX
:10 »Q   or more shall be put through between the terminal
and the shaft at 250 VDC mega.
:No abnormality shall be observed after lOOVAC is
impressed for one minute between the terminal and the shaft.

is impressed  on anode. )	/ISS	_-
4- 9  Direction of revolution	:CW, CCW (CW seen from the output shaft when t power
!!E_D

5   CONDITIONS

I  N	U S E	(

5-1 Range of Temperature in use  :-10 ·c- +  60  ·c	SfPOZ.   1997	)
5-2 Range of storing temperature :-15 ·c - + 65 ·c	ht=-	· ""-4Q:/
5-3 Mounting posture 	:Output shaft horizontal direction 	£.aSID A;v-Y

6   SPECIFICATIONS FOR PACKING
Packing shall be done so that no damage may be done during transportation.	, 	fjt

7   ADDITIONAL 	REMARKS
Any specification not given in this specifications shall be determined by
mutual consultation.

8   GREASE D-300

M,\tll 02- 2

DATE
A L T

2. AUG. 97' 	Recognize	S.HJ\$111 tOTO
6J 	Draw up	K.llaeno
AVAMA	P "J;"rt T()l\J 	Tl\JllTT 'T' T"J;"	('() 	T      1''"' .