INTRODUCTION:
CASA’s light-gauge folded steel PATCH Panels are designed to meet the budget-consious requirements of the videa, security and small-scale professional and industrial electronics Industry for high-precision quality 19" PATCH Panels for incorporation into equipment racks and cabinets where PROFESSIONAL appearance and LOW weight are required. These Channel-profile panels are designed with varing standard densities up to 24 connectors per 1RU (one rack unit height of 44.45mm), 

FEATURES:
1) Standard UNIT heights (1U = 44.45mm=1.75") from 1-2 units (3 to 6 Unit and larger panels can be made to order).
3) Simple channel and angle design gives high strength and permits standard & SPECIAL, finishes and variants to be
produced economically even in small quantities with features including custom punchings to suit a wide range of coaxial, audio
and data connectors
4) Optional lacing bars can be installed or retrofitted to most panels to ensure that tensional loading of cables is safely absorbed.
5) Laser engraved legends are economicaly applied using simple numbering or custom nomenclature.

Footer:
PROFESSIONAL QUALITY IN COMPUTER & ELECTRONIC HARDWARE, COMPONENTS & MATERIALS

Part Numbering Composition:

Part Number:- PP-xU-yyWZZ-ALg-F(special adder/suffix)

PP = Prefix to indicate "PATCH PANEL".
xxU = HEIGHT in RACK Units (multiples of 44.45 millimeters).
yyW = number of ways, W = Ways
p = Pattern designation if not in a straight line
zz = Connector type/family designation
MSg = Mild-steel where "g" GAUGE of stock material in "mm"
F = FINISH applied (MB = MatBlack; N=Natural; ZC=Zinc-Plated + Chrome-Passivation
(------) = Special adder or suffix gives Custom information or Drawing No etc for unique reference.

Please compose a Part Number according to this system and use on your official order.