ContentsPreviousNext
Settings

# Specifying the scanning side according to the original (Type 2 model)

If you are using the Type 2 model, you can specify the machine to scan both sides of original automatically using the ARDF.

This section describes how to specify the scanning side according to the current original.

Press [Original].

Press the [][] keys to select the desired scanning method, and then press the [OK] key.

Select the sides of the original (1 side or 2-sides) to scan. When scanning 2-sides, select the page and binding orientations according to the original.

- You can press the [Escape] key to exit to the previous level of the menu tree.

- If 2-sided scanning is specified, you must use the ARDF (scanning will not be possible with the exposure glass).

- You can change the machine's default [Original] setting to always scan specific sides of originals.

- Temporary job settings are cleared in the following cases:

  - When no input is received for the period of time specified in [System Auto Reset Timer] while the initial screen is displayed.

  - When the [Clear/Stop] key is pressed while the initial screen is displayed.

  - When the machine's mode is changed.

  - When the power is turned off.

  - When the machine's default for the same setting is changed.

- For details about [Original], see Scanner Settings.

- For details about [System Auto Reset Timer], see Administrator Settings.