ContentsPreviousNext
Settings

# Unpacking

To protect it from shock and vibration during transit, this machine comes packaged in cushioning foam and secured with tape. Remove these protective materials after bringing the machine to where it will be installed.

| Be sure to locate the machine as close as possible to a wall outlet. This will allow easy disconnection of the power cord in the event of an emergency.

| If the machine emits smoke or odours, or if it behaves unusually, you must turn off its power immediately. After turning off the power, be sure to disconnect the power cord plug from the wall outlet. Then contact your service representative and report the problem. Do not use the machine. Doing so could result in fire or electric shock.

| If metal objects, or water or other fluids fall inside this machine, you must turn off its power immediately. After turning off the power, be sure to disconnect the power cord plug from the wall outlet. Then contact your service representative and report the problem. Do not use the machine. Doing so could result in fire or electric shock.

| Do not touch this machine if a lightning strike occurs in the immediate vicinity. Doing so could result in electric shock.

| The following explains the warning messages on the plastic bag used in this product's packaging. Keep the polythene materials (bags, etc.) supplied with this machine away from babies and small children at all times. Suffocation can result if polythene materials are brought into contact with the mouth or nose.

| Do not incinerate toner (new or used) or toner containers. Doing so risks burns. Toner will ignite on contact with naked flame.

| Do not store toner (new or used) or toner containers anywhere near naked flames. Doing so risks fire and burns. Toner will ignite on contact with naked flame.

| Do not use the cleaner to suck spilled toner (including used toner). Sucked toner may cause firing or explosion due to electrical contact flickering inside the cleaner. However, it is possible to use the cleaner designed for dust explosion-proof purpose. If toner is spilled over the floor, sweep up spilled toner slowly and clean remainder with wet cloth.

| Do not crush or squeeze toner containers. Doing so can cause toner spillage, possibly resulting in dirtying of skin, clothing, and floor, and accidental ingestion.

| Store toner (new or used), toner containers, and components that have been in contact with toner out of reach of children.

| If toner or used toner is inhaled, gargle with plenty of water and move into a fresh air environment. Consult a doctor if necessary.

| If toner or used toner gets into your eyes, flush immediately with large amounts of water. Consult a doctor if necessary.

| If toner or used toner is swallowed, dilute by drinking a large amount of water. Consult a doctor if necessary.

| When moving the machine, use the inset grips on both sides. The machine will break or cause injury if dropped.

| Do not look into the lamp. It can damage your eyes.

| During operation, rollers for transporting the paper and originals revolve. A safety device has been installed so that the machine can be operated safety. But take care not to touch the machine during operation. Otherwise, an injury might occur.

- Removed tape is dirty. Be careful not to let it touch your hands or clothes.

- Leave the protective materials in place while moving the machine.

- Lower the machine slowly and carefully to prevent trapping your hands.

- Do not grip on the tray area when lifting the machine.

- Do not allow paper clips, staples, or other small objects to fall inside the machine.

- Keep uncovered print cartridge away from direct sunlight.

- Do not touch the print cartridge's photo conductor unit.

- Do not touch the ID chip on the side of the print cartridge as indicated in the illustration below.

Remove the plastic bag.

Lift the machine by using the inset grips on both sides of the machine.

Remove the protective materials attached on the machine's exterior.

Be sure to also remove the protective sheet on the control panel.

The actual machine may come with protective materials attached in different positions. Make sure to check the machine's exterior for all protective materials, and remove them completely.

Open the ADF cover.

Gently pull the protective sheet to remove it.

Close the ADF cover.

Remove the protective sheet and materials.

Open the rear cover, and then peel off the tape on both sides of the machine.

Pull out the tapes and remove the protective materials. Doing so will pull up the levers on both sides.

Check that the levers have been pulled up to the positions indicated with . If not, pull them up completely manually.

Leaving the levers lowered or not pulled up completely may affect the print quality, as toner may be insufficiently fused.

Close the rear cover.

Push the side button to open the front cover, and then carefully lower it.

Remove the protective material attached inside the machine.

Unpack the print cartridge. Then, place it on a flat surface, and remove the protection sheet.

Shake the print cartridge from side to side five or six times.

Slide the print cartridge in horizontally. When the cartridge can go no further, raise it slightly and push it fully in. Then push down on the cartridge until it clicks into place.

Using both hands, carefully push up the front cover until it closes.

Carefully pull tray 1, and then pull out with both hands.

Place the tray on a flat surface.

Remove the protective material attached inside the tray.

Carefully push tray 1 straight into the machine.

Pull out and raise the stop fence.