ContentsPreviousNext
Settings

# Multi-access

This machine can perform multiple jobs using different functions, such as copying and faxing, at the same time. Performing multiple functions simultaneously is called “Multi-access”.

The following table shows the functions that can be performed simultaneously.

Current job | Job that you want to execute simultaneously
--- | ---
Copying | Fax memory transmission Fax memory reception Internet Fax reception (no printing) Receiving a print job from a computer (the actual printing starts after copying is finished) Receiving a LAN-Fax job from a computer LAN-Fax transmission
Scanning | Fax memory transmission Fax immediate printing Fax memory reception Printing a fax received in the machine's memory Internet Fax reception Printing Receiving a LAN-Fax job from a computer LAN-Fax transmission
Scanning a fax into the machine's memory before transmission | Fax memory transmission Fax immediate printing Fax memory reception Printing a fax received in the machine's memory Internet Fax reception Printing Receiving a LAN-Fax job from a computer LAN-Fax transmission
Fax immediate transmission (scanning an original and sending it simultaneously) | Printing a fax received in the machine's memory Internet Fax reception Printing Receiving a LAN-Fax job from a computer
Fax memory transmission (sending a fax that has already been stored in the machine's memory) | Copying Scanning Scanning a fax into the machine's memory before transmission Internet Fax transmission Printing a fax received in the machine's memory Internet Fax reception Printing Receiving a LAN-Fax job from a computer
Internet Fax transmission | Fax memory transmission Fax immediate printing Fax memory reception Printing a fax received in the machine's memory Printing Receiving a LAN-Fax job from a computer LAN-Fax transmission
Fax immediate printing (receiving a fax and printing it simultaneously) | Scanning *1 Scanning a fax into the machine's memory before transmission Internet Fax transmission Internet Fax reception (no printing) Receiving a LAN-Fax job from a computer
Fax memory reception (storing a received fax into the machine's memory) | Copying Scanning Scanning a fax into the machine's memory before transmission Internet Fax transmission Internet Fax reception (no printing) Receiving a LAN-Fax job from a computer
Printing a fax received in the machine's memory | Scanning *1 Scanning a fax into the machine's memory before transmission Fax immediate transmission Fax memory transmission Internet Fax transmission Internet Fax reception (no printing) Receiving a LAN-Fax job from a computer LAN-Fax transmission
Internet Fax reception | Copying (except when printing out the received Internet Fax) Scanning Scanning a fax into the machine's memory before transmission Fax immediate transmission Fax memory transmission Fax immediate printing (except when printing out the received Internet Fax) Fax memory reception (except when printing out the received Internet Fax) Printing a fax received in the machine's memory (except when printing out the received Internet Fax) Printing (except when printing out the received Internet Fax) Receiving a LAN-Fax job from a computer LAN-Fax transmission
Printing | Scanning Scanning a fax into the machine's memory before transmission Fax immediate transmission Fax memory transmission Internet Fax transmission Internet Fax reception (no printing) LAN-Fax transmission
Receiving a LAN-Fax job from a computer | Copying Scanning Fax immediate printing Fax memory reception Printing a fax received in the machine's memory Internet Fax reception LAN-Fax transmission
LAN-Fax transmission | Copying Scanning Scanning a fax into the machine's memory before transmission Internet Fax transmission Printing a fax received in the machine's memory Internet Fax reception Printing Receiving a LAN-Fax job from a computer

*1 Fax printing may take longer than normal if you scan using the control panel at the same time, especially when scanning multiple pages using the exposure glass.

- If you try to use a function that cannot be performed simultaneously, you will hear a beep sound from the machine or see a failure message pop up on your computer screen. In this case, try again after the current job is finished.