ContentsPreviousNext
Settings

# Useful Sending Functions

This section explains some useful fax functions.

You can confirm the status of the other party's machine easily before sending a fax by using the On Hook Dial function. If you have an extra telephone, you can talk and send a fax in one call.

- This function is available in Immediate Transmission mode only.

- This function is not available with Internet Fax.

- For details about selecting the transmission mode, see Selecting Transmission Mode.

Related topics

Sending a fax using On Hook Dial
Sending a fax after a conversation