ContentsPreviousNext
Settings

# Specifying the resolution

This section describes how to specify the scan resolution for the current job.

There are three resolution settings:

Standard

Select this when the original is a printed or typewritten document with normal-sized characters.

Detail

Select this when the original is a document with small print.

Photo

Select this when the original contains images such as photographs or shaded drawings.

Press the [Image Quality] key.

Press the [][] keys to select the desired resolution setting, and then press the [OK] key.

- Press the [Escape] key to discard the current change and return to the initial screen.

- You can change the machine's default [Resolution] setting to always scan with a specific resolution level.

- The `“Photo”` resolution is not available for Internet Faxes. Faxes will be sent using `“Detail”` resolution if `“Photo”` resolution has been specified.

- Temporary job settings are cleared in the following cases:

  - When no input is received for the period of time specified in [System Auto Reset Timer] while the initial screen is displayed.

  - When the [Clear/Stop] key is pressed while the initial screen is displayed.

  - When the machine's mode is changed.

  - When the power is turned off.

  - When the machine's default for the same setting is changed.

- For details about [Resolution], see Fax Transmission Settings.

- For details about [System Auto Reset Timer], see Administrator Settings.