ContentsPreviousNext
Settings

# Scanner Function Specifications

Maximum scanning area (horizontal × vertical)

- Exposure glass

  216 × 297 mm (8.5 × 11.7 inches)

- ARDF/ADF

  216 × 356 mm (8.5 × 14.1 inches)

Maximum resolution when scanning from the control panel (Scan to E-mail, Scan to FTP, Scan to Folder, Scan to USB)

- Exposure glass

  600 × 600 dpi

- ARDF/ADF

  600 × 600 dpi

Maximum resolution when scanning from a computer (TWAIN)

- Exposure glass

  19200 × 19200 dpi

- ARDF/ADF

  600 × 600 dpi

Maximum resolution when scanning from a computer (WIA)

- Exposure glass

  600 × 600 dpi

- ARDF/ADF

  600 × 600 dpi

Gradation

Input: 16 bit color processing

Output: 8 bit color processing

Scanning time (600 dpi)

Black and white: 5 seconds or less

Color: 10 seconds or less

Not including transfer time.

ARDF/ADF throughput (300 dpi)

Black and white: 120 mm per second

Color: 60 mm per second

Interface

- Scanning from the control panel

  Ethernet (10BASE-T, 100BASE-TX), USB2.0 (Scan to USB)

- Scanning from a computer

  Ethernet (10BASE-T, 100BASE-TX), USB 2.0

Sendable file formats

TIFF, JPEG, PDF

Address book

Maximum 100 items

Number of redials: 1