ContentsPreviousNext
Settings

# Cleaning the Friction Pad and Paper Feed Roller

If the friction pad or paper feed roller is dirty, a multi-feed or jam might occur. In this case, clean the friction pad and paper feed roller as follows:

| Unplug the power cord from the wall outlet before you move the machine. While moving the machine, take care that the power cord is not damaged under the machine. Failing to take these precautions could result in fire or electric shock.

| Do not pull out the paper tray forcefully. If you do, the tray might fall and cause an injury.

| Do not put your hands inside the machine when the input tray is removed. Some internal parts become hot and are a burn hazard.

- Do not use chemical cleaning fluids or organic solvents such as thinner or benzine.

Turn off the power.

Unplug the power cord from the wall outlet. Remove all the cables from the machine.

Pull out tray 1 carefully with both hands.

Place the tray on a flat surface. If there is paper in the tray, remove it.

Wipe the friction pads with a damp cloth.

Wipe the rubber part of the roller with a soft damp cloth. After that, wipe it with a dry cloth to remove the moisture.

Reload the removed paper into the tray, and then push the tray carefully into the machine until it clicks into place.

Insert the plug of the power cord into the wall socket securely. Connect all the interface cables that were removed.

Turn on the power.

- If jams or multi-sheet feeds occur after cleaning the friction pad, contact your sales or service representative.

- If the optional tray 2 is installed, clean its friction pad and paper feed roller in the same way as you did for tray 1.