ContentsPreviousNext
Settings

# Removing Printing Jams

If a paper jam occurs, one of the following messages appears on the screen:

- "Misfeed: Bypass Tray"

- "Misfeed: Dup. Unit Remove Paper"

- "Internal Misfeed"

- "Misfeed: Stnd. Tray"

- "Misfeed: Tray 1"

- "Misfeed: Tray 2"

- Jammed paper may be covered in toner. Be careful not to get toner on your hands or clothes.

- Toner on prints made immediately after clearing a paper jam may be insufficiently fused and can smudge. Make test prints until smudges no longer appear.

- Do not forcefully remove jammed paper, as it may tear. Torn pieces remaining inside the machine will cause further jams and possibly damage the machine.

- Paper jams can cause pages to be lost. Check your print job for missing pages and reprint any pages that did not print out.

Related topics

Removing internal/tray 1/tray 2 jam
Removing bypass tray jam
Removing standard tray/duplex unit jam