ContentsPreviousNext
Settings

# Sending faxes from a computer (LAN-Fax)

You can send a document directly from a computer through this machine to another fax machine, without printing the document.

- This function is supported by Windows XP/Vista/7, and Windows Server 2003/2003 R2/2008/2008 R2. Mac OS X does not support this function.

Preparation for sending faxes from a computer connected via USB

1. Connect the machine to a computer using a USB cable.

   For details, see Connecting with a Computer Using a USB Cable.

2. Install the LAN-Fax driver on the computer.

   For details, see the instructions provided on the driver CD-ROM.

3. Register LAN-Fax destinations in the LAN-Fax Address Book.

   For details, see Configuring the LAN-Fax Address Book.

Preparation for sending faxes from a computer connected via network

1. Connect the machine to the network.

   For details, see Connecting with a Network Cable.

2. Specify the network settings, such as the machine’s IP address.

   For details, see Configuring the Machine.

3. Install the LAN-Fax driver on the computer.

   For details, see the instructions provided on the driver CD-ROM.

4. Register LAN-Fax destinations in the LAN-Fax Address Book.

   For details, see Configuring the LAN-Fax Address Book.