ContentsPreviousNext
Settings

# Placing originals on the exposure glass

The exposure glass enables you to scan and send documents that cannot be fed into the ARDF or ADF.

- Do not lift the ARDF or ADF forcefully. Otherwise, the cover of the ARDF or ADF might open or be damaged.

Lift the ARDF or ADF.

Be careful not to hold the input tray when lifting the ARDF or ADF, for the tray might be damaged.

Place the original face down on the exposure glass. The original should be aligned to the rear left corner.

Lower the ARDF or ADF.

Hold down the ARDF or ADF with your hands when using thick, folded, or bound originals and the ARDF or ADF cannot be lowered completely.