ContentsPreviousNext
Settings

# Selecting Transmission Mode

This section describes how to select the transmission mode.

There are two transmission modes: Memory Transmission and Immediate Transmission.

Memory Transmission

In this mode, the machine scans several originals into memory and sends them all at once. This is convenient when you are in a hurry and want to take the document away from the machine. In this mode, you can send a fax to multiple destinations.

Select this mode when scanning 2-sides of original and send them using the ARDF with the Type 2 model.

Immediate Transmission

In this mode, the machine scans the original and faxes it simultaneously, without storing it in memory. This is convenient when you want to send an original quickly. In this mode, you can only specify one destination.

Note that if the machine is in this mode, only one side of the original is scanned using the ARDF regardless of the ARDF original setting for the Type 2 model.

Press the [Facsimile] key, and then press the [][] keys.

Alternatively, you can press the [Shortcut to Func.] key if [Shortcut to Function] under administrator settings is set to [Fax Immediate TX].

Press the [][] keys to select [Immediate TX], and then press the [OK] key.

Press the [][] keys to select [Off], [On], or [Next Fax Only], and then press the [OK] key.

For Memory Transmission, select [Off].

For Immediate Transmission, select [On] or [Next Fax Only].

Press the [User Tools] key to return to the initial screen.

- You can press the [Escape] key to exit to the previous level of the menu tree.

- For details about [Shortcut to Function], see Administrator Settings.