ContentsPreviousNext
Settings

# Basic Operation for Sending a Fax

This section describes the basic operation for sending a fax.

- The original in the ARDF or ADF takes precedence over the original on the exposure glass if you place originals both in the ARDF/ADF and on the exposure glass.

Press the [Facsimile] key.

Place the original on the exposure glass or in the ARDF/ADF.

If necessary, configure the advanced scan settings.

Enter the fax number (up to 40 characters) using the number keys, or specify a destination using the One Touch buttons or Speed Dial function.

- If the machine is connected to the telephone network through a PBX, make sure to enter the outside line access number specified in [PBX Access Number] before the fax number.

- To specify an Internet Fax destination, use the One Touch buttons or Speed Dial function.

Press the [Start] key.

- Depending on the machine's settings, you may be prompted to enter the fax number again if you manually entered the destination fax number. In this case, re-enter the number within 30 seconds, press [OK], and then press the [Start] key. If the fax numbers do not match, go back to step 3.

- When using the exposure glass in Memory Transmission mode, you will be prompted to place another original. In this case, proceed to the next step.

If you have more originals to scan, press [Yes] within 60 seconds, place the next original on the exposure glass, and then press [OK]. Repeat this step until all originals are scanned.

If you do not press [Yes] within 60 seconds, the machine will start to dial the destination.

When all originals have been scanned, press [No] to start sending the fax.

- A fax number can contain 0 to 9, pause, "", "", and space.

- If necessary, insert a pause in a fax number. The machine pauses briefly before it dials the digits following the pause. You can specify the length of the pause time in the [Pause Time] setting under fax transmission settings.

- To use tone services on a pulse-dialing line, insert "" in a fax number. "" switches the dialing mode from pulse to tone temporarily.

- You can also specify a destination from an LDAP server or with the [Pause/Redial] key.

- You can specify multiple destinations and broadcast the fax you are sending.

- The machine prompts you to enter the fax number twice only when you dial the destination manually. Destinations specified using the One Touch buttons, Speed Dial function, or [Pause/Redial] key need not be confirmed.

- When in Memory Transmission mode, you can enable the [Auto Redial] setting under fax transmission settings to set the machine to automatically redial the destination if the line is busy or an error occurs during transmission.

- When in Memory Transmission mode, the machine's memory may become full while scanning the originals. In this case, the screen prompts you to cancel the transmission or to send only the pages that have been scanned successfully.

- If you specify an Internet Fax destination in Immediate Transmission mode, the mode switches to Memory Transmission mode temporarily.

- If paper is jammed in the ARDF or ADF, the jammed page has not been scanned properly. When the machine is in Immediate Transmission mode, resend the fax starting from the jammed page. When in Memory Transmission mode, scan the entire originals again.

- For details about entering characters, see Entering Characters.

- To place the originals, see Placing Originals.

- To configure advanced scan settings, see Specifying the Scan Settings.

- For details about [PBX Access Number], see Administrator Settings.

- For details about specifying destinations using the One Touch buttons, Speed Dial function, LDAP server, or [Pause/Redial] key, see Specifying the Fax Destination.

- For details about broadcasting a fax, see Specifying the Fax Destination.

- For details about fax number confirmation, see Administrator Settings.

- For details about [Auto Redial] or [Pause Time], see Fax Transmission Settings.

- For details about how to remove the paper jammed in the ADF or ARDF, see Removing Scanning Jams (Type 2 model) or Removing Scanning Jams (Type 1 model).

Related topics

Canceling a fax