ContentsPreviousNext
Settings

# Combining Pages and Making 2-sided Copies

This section describes how to set the machine to combine multiple pages (2 or 4 pages) of an original onto a single page. Also, with the Type 2 model, you can scan 2-sided originals and make 2-sided copies.

- This function is only available when the original is set in the ARDF or ADF, not when it is set on the exposure glass.

- For combine and 2-sided copying, the paper size must be A4, Letter or Legal.

- For 2-sided copying, the paper type must be thin, plain, recycled, color, preprinted, prepunched, thick paper 1, or letterhead.

There are following copy modes. Select a copy mode according to your original and how you want the copy outputs to appear.

Combined copy on 1 side

In this mode, copy will be made on 1 side, on which 2 or 4 pages of an original will be printed.

- 1Sd 2Orig->Comb 2on1 1Sd

- 1Sd 4Orig->Comb 4on1 1Sd

- 2Sd 1Orig->Comb 2on1 1Sd (Type 2 model only)

- 2Sd 2Orig->Comb 4on1 1Sd (Type 2 model only)

Combined copy on 2 sides (Type 2 model only)

In this mode, copy will be made on 2 sides, on each of which 2 or 4 pages of an original will be printed.

- 1Sd 4Orig->Comb 2on1 2Sd

- 1Sd8Orig->Comb 4on1 2Sd

- 2Sd 2Orig->Comb 2on1 2Sd

- 2Sd 4Orig->Comb 4on1 2Sd

Copy on 2 sides (Type 2 model only)

In this mode, copy will be made on 2 sides, on each of which a single page of an original will be printed.

- 1 Sided Orig->2 Sided Copy

- 2 Sided Orig->2 Sided Copy

Use this procedure to set copy mode for the current job.

Press [Dup/Comb].

Alternatively, you can press the [Shortcut to Func.] key if [Shortcut to Function] under administrator settings is set to [Dup/Comb Copy].

Press the [][] keys to select the desired copy mode, and then press the [OK] key.

Press the [][] keys to select page and binding orientations, and then press the [OK] key.

The screen will show the selected copy mode.

- You can press the [Escape] key to exit to the previous level of the menu tree.

- You can change the machine's default [Duplex/Combine] setting to always make photocopies in combine/2-sided mode.

- Setting combined/2-sided copying automatically disables the [ID Card Copy] setting.

- Temporary job settings are cleared in the following cases:

  - When no input is received for the period of time specified in [System Auto Reset Timer] while the initial screen is displayed.

  - When the [Clear/Stop] key is pressed while the initial screen is displayed.

  - When the machine's mode is changed.

  - When the power is turned off.

  - When the machine's default for the same setting is changed.

- For details about [Shortcut to Function], see Administrator Settings.

- For details about [Duplex/Combine], see Copy Settings.

- For details about [System Auto Reset Timer], see Administrator Settings.

- To make 2-sided copies with the Type 1 model, perform manual duplex copying. See Making 2-sided Copies Manually (Type 1 model).