ContentsPreviousNext
Settings

# Settings you can configure in the LAN-Fax driver's properties

This section describes the settings you can configure in the LAN-Fax driver's properties.

1. Paper Size

   Specifies the paper size.

   - Document Size

     Specifies the paper size of the document you are sending. If a paper size is specified in the application, that paper size will be used. Otherwise, the paper size specified here will be used.

   - Sending Size:

     Displays the actual paper size of the fax that is sent. The actual size of the fax will be A4, if the size of the document being faxed is A3, B4, or smaller than A4. A3/B4 documents will be reduced to sending size automatically.

2. Orientation

   Specifies the page orientation.

3. Resolution

   Specifies the resolution.

   - Standard

     Select this for a document with normal-sized characters.

   - Fine

     Select this for a document with small print.

   - Photo

     Select this for a document with images such as photographs or shaded drawings.

4. User Code

   If sending faxes via LAN-Fax is restricted, select this check box and enter a user code before sending a fax.

5. Authentication

   If LDAP authentication is specified, click this button to enable user authentication and enter a user name and password before sending a fax job to the machine.

6. About...

   Displays the version of the LAN-Fax driver.

7. Restore Defaults

   Restores the settings to their factory defaults.

- The settings configured here are applicable for the current application only.