ContentsPreviousNext
Settings

# Configuring Transmission Settings

This section describes how to configure transmission settings in the LAN-Fax driver's properties.

Properties are set separately for each application.

On the [File] menu, click [Print...].

Select the LAN-Fax driver as the printer, and then click a button such as [Preferences] or [Properties] to open the driver's properties.

LAN-Fax driver properties dialog box appears.

Click the [Setup] tab.

Configure settings as necessary, and then click [OK].

- For details about settings, see Settings you can configure in the LAN-Fax driver's properties.

Related topics

Settings you can configure in the LAN-Fax driver's properties