ContentsPreviousNext
Settings

# Assigning the machine's IPv4 address manually

- The IPv4 address assigned to the machine must not be used by any other device on the same network.

Press the [User Tools] key.

Press the [] [] keys to select [Network Settings], and then press the [OK] key.

If you are requested to enter a password, enter the password using the number keys, and then press the [OK] key.

Press the [] [] keys to select [IPv4 Configuration], and then press the [OK] key.

Press the [] [] keys to select [DHCP], and then press the [OK] key.

Press the [] [] keys to select [Inactive], and then press the [OK] key.

Press the [] [] keys to select [IP Address], and then press the [OK] key.

The current IPv4 address is shown.

Enter the machine’s IPv4 address using the number keys, and then press the [OK] key.

Press the [] [] keys to move between fields.

Press the [] [] keys to select [Subnet Mask], and then press the [OK] key.

The current subnet mask is shown.

Enter the subnet mask using the number keys, and then press the [OK] key.

Press the [] [] keys to move between fields.

Press the [] [] keys to select [Gateway Address], and then press the [OK] key.

The current gateway address is shown.

Enter the gateway address using the number keys, and then press the [OK] key.

Press the [] [] keys to move between fields.

Press the [User Tools] key to return to the initial screen.

If you are requested to restart the machine, turn off the machine, and then turn it back on.

Print the configuration page to confirm the setting.

The IPv4 address setting will appear under “TCP/IP” on the configuration page.

- You can press the [Escape] key to exit to the previous level of the menu tree.

- A password for accessing the [Network Settings] menu can be specified in [Admin. Tools Lock].

- If your network environment requires a specific transmission speed that is not automatically detected, set the transmission speed in [Set Ethernet Speed] under [Network Settings].

- When [DHCP] is activated, manually configured IPv4 address settings are not used.

- For details about turning the machine on and off, see Turning the Power on.

- For details about printing configuration page, see Printing the Configuration Page.

- For details about [Admin. Tools Lock], see Administrator Settings.

- For details about [Set Ethernet Speed], see Configuring the Ethernet Speed.