ContentsPreviousNext
Settings

# Moving the Machine

This section provides cautions that you must follow when moving the machine both short and long distances.

| If you have to move the machine when the optional paper tray unit is attached, do not push on the main unit's top section. Doing so can cause the optional paper tray unit to detach, possibly resulting in injury.

| The machine weighs approximately 18.4 kg (40.6 lb.). When moving the machine, use the inset grips on both sides, and lift slowly. The machine will break or cause injury if dropped.

| Unplug the power cord from the wall outlet before you move the machine. While moving the machine, take care that the power cord is not damaged under the machine. Failing to take these precautions could result in fire or electric shock.

| When disconnecting the power cord from the wall outlet, always pull the plug, not the cord. Pulling the cord can damage the power cord. Use of damaged power cords could result in fire or electric shock.

| When moving the machine after use, do not take out the toner to prevent toner spill inside the machine.

Repack the machine in its original packing materials when moving it a long distance.

- Be sure to disconnect all cables from the machine before transporting it.

- The machine is a precision piece of machinery. Be sure to handle it carefully when moving it.

- Make sure to move the machine horizontally. Take extra caution when carrying the machine up or down stairs.

- If tray 2 is installed, remove it from the machine, and move them separately.

- Do not hold onto the tray area when lifting the machine.

Related topics

Moving over a Short Distance
Moving over a Long Distance