ContentsPreviousNext
Settings

# Removing internal/tray 1/tray 2 jam

If `“Internal Misfeed”`, `“Misfeed: Tray 1”`, `“Misfeed: Tray 2”` appears on the display, follow the procedure below to remove it.

| The inside of this machine becomes very hot. Do not touch the parts labeled "" (indicating a hot surface).

| Some of this machine's internal components get very hot. For this reason, take care when removing misfed paper. Not doing so could result in burns.

| When removing jammed paper, make sure not to trap or injure your fingers.

Pull tray 1 halfway out, and check for jammed paper. If there is jammed paper, remove it carefully.

Carefully slide tray 1 back in until it stops.

If paper is loaded in the bypass tray, remove the paper.

Close the bypass tray.

Push the side button to open the front cover, and then carefully lower it.

Carefully pull out the print cartridge horizontally, holding its center.

- Do not shake the removed print cartridge. Doing so can cause remaining toner to leak.

- Place the print cartridge on paper or similar material to avoid dirtying your workspace.

Lifting the guide plate, remove the jammed paper carefully.

Slide the print cartridge in horizontally. When the cartridge can go no further, raise it slightly and push it fully in. Then push down on the cartridge until it clicks into place.

Using both hands, carefully push up the front cover until it closes.

- If paper is jammed in tray 2 but is difficult to locate, pull out tray 2 to remove it. After removing the paper, carefully push tray 2 all the way back inside the machine.

- When closing the front cover, push the upper area of the cover firmly. After closing the cover, check that the error is cleared.