ContentsPreviousNext
Settings

# Specifying the destination using the broadcast function

You can send a fax to multiple destinations simultaneously. You can broadcast faxes to a maximum of 100 destinations (including both normal fax destinations and Internet Fax destinations).

Faxes are sent to destinations in the order they were specified.

Press the [Facsimile] key.

Add a destination by using one of the following methods:

- To add a Quick Dial destination: press a corresponding One Touch button.

- To add a Speed Dial destination: press the [Address Book] key, select [Search Address Book], select a destination, and then press the [OK] key.

- To add a manually-specified destination: confirm that [No.key] is pressed, and then enter the destination fax number using the number keys.

- To add a destination from an LDAP server: follow the procedure in "Specifying the destination from an LDAP server".

Press the [OK] key.

Press [List] to see the list of destinations that have been added so far.

Go back to step 2 to add further destinations.

- While specifying multiple destinations, you can press the [Clear/Stop] key to clear all destinations.

- If you specify multiple destinations in Immediate Transmission mode, the mode switches to Memory Transmission mode temporarily.

- If the destinations contain both normal fax destinations and Internet Fax destinations, the fax will be sent to the Internet Fax destinations first.

- While broadcasting, pressing the [Clear/Stop] key cancels the fax to the current destination only.

- For details about specifying a destination from an LDAP server, see Specifying the destination from an LDAP server.