ContentsPreviousNext
Settings

# Setting the outside line access number

If the machine is connected to the telephone network through a PBX, set the dial number to access the outside line.

- Make sure to set the outside line access number that matches the setting of your PBX. Otherwise, you may not be able to send faxes to outside destinations.

Press the [User Tools] key.

Press the [] [] keys to select [Admin. Tools], and then press the [OK] key.

If you are requested to enter a password, enter the password using the number keys, and then press the [OK] key.

Press the [] [] keys to select [PBX Access Number], and then press the [OK] key.

Enter the outside line access number using the number keys, and then press the [OK] key.

Press the [User Tools] key to return to the initial screen.

- You can press the [Escape] key to exit to the previous level of the menu tree.

- A password for accessing the [Admin. Tools] menu can be specified in [Admin. Tools Lock].

- For details about [Admin. Tools Lock], see Administrator Settings.