ContentsPreviousNext
Settings

# Sending a fax using On Hook Dial

The On Hook Dial function allows you to check the destination's status while listening to the tone from the internal speaker. This function is useful when you want to ensure that the fax will be received.

- The On Hook Dial function cannot be used when [Fax Number Confirmation] under administrator settings is enabled.

Place the original.

Press the [Facsimile] key.

Press the [On Hook Dial] key.

`“On Hook”` appears on the screen.

Specify the destination using the number keys.

If you hear a high pitched tone, press the [Start] key.

Press [TX], and then press the [Start] key.

- For details about [Fax Number Confirmation], see Administrator Settings.