ContentsPreviousNext
Settings

# Unscannable image area

Even if you correctly place originals in the ARDF or ADF or on the exposure glass, margins of a few millimeters on all four sides of the original might not be scanned.

Margins when using exposure glass
| In copier mode | In scanner mode | In fax mode
--- | --- | --- | ---
Top | 4 mm | 0 mm | 1 mm
Right | 3 mm | 0 mm | 1 mm
Left | 3 mm | 0 mm | 1 mm
Bottom | 4 mm | 0 mm | 2 mm

Margins when using ARDF or ADF
| In copier mode | In scanner mode | In fax mode
--- | --- | --- | ---
Top | 4 mm | 0 mm | 0 mm
Right | 3 mm | 0 mm | 1 mm
Left | 3 mm | 0 mm | 1 mm
Bottom | 4 mm | 0 mm | 2 mm