ContentsPreviousNext
Settings

# Network Setting Parameters

This section describes the network setting parameters.

Ethernet

- MAC Address

  Displays the machine's MAC address.

- Ethernet Speed

  Displays the current Ethernet speed setting.

  - 100Mbps Full Duplex

  - 100Mbps Half Duplex

  - 10Mbps Full Duplex

  - 10Mbps Half Duplex

  - Ethernet Unavailable

    Appears when a network cable is not connected.

- Set Ethernet Speed

  Specifies the speed for Ethernet communication. Select a speed that matches your network environment.

  For most networks, the default setting is the optimum setting.

  Default: [Auto Select]

  - Auto Select

  - 100Mbps Full Duplex

  - 100Mbps Half Duplex

  - 10Mbps Full Duplex

  - 10Mbps Half Duplex

IPv4 Configuration

- DHCP

  Sets the machine to receive its IPv4 address, subnet mask, and default gateway address automatically from a DHCP server.

  Default: [Active]

  - Active

  - Inactive

- IP Address

  Specifies the machine's IPv4 address when DHCP is not used.

  Use this menu to check the current IP address when DHCP is used.

  Default: XXX.XXX.XXX.XXX

  The numbers represented by "X" vary according to your network environment.

- Subnet Mask

  Specifies the machine's subnet mask when DHCP is not used.

  Use this menu to check the current subnet mask when DHCP is used.

  Default: XXX.XXX.XXX.XXX

  The numbers represented by "X" vary according to your network environment.

- Gateway Address

  Specifies the machine's default gateway address when DHCP is not used.

  Use this menu to check the current default gateway address when DHCP is used.

  Default: XXX.XXX.XXX.XXX

  The numbers represented by "X" vary according to your network environment.

- IP Address Method

  Displays the IP address acquisition method.

  - DHCP

  - Auto IP

  - Manual Config.

  - Default IP

IPv6 Configuration

- IPv6

  Select whether to enable or disable IPv6.

  Default: [Active]

  - Active

  - Inactive

- DHCP

  Sets the machine to receive its IPv6 address from a DHCP server.

  Default: [Inactive]

  - Active

  - Inactive

- IP Address (DHCP)

  Displays the IPv6 address obtained from a DHCP server.

- Manual Config. Address

  - Manual Config. Address

    Specifies the machine's IPv6 address when DHCP is not used. Can contain up to 39 characters.

    For details about entering characters, see Entering Characters.

  - Prefix Length

    Specifies the prefix length, using a value between 0 and 128.

  - Gateway Address

    Specifies the IPv6 address of the default gateway. Can contain up to 39 characters.

    For details about entering characters, see Entering Characters.

- Stateless Address

  Displays the IPv6 stateless addresses obtained from a Router Advertisement.

  - Stateless Address 1

  - Stateless Address 2

  - Stateless Address 3

  - Stateless Address 4

- Link-local Address

  Displays the IPv6 link local address.

- Contact your network administrator for information about the network configuration.