ContentsPreviousNext
Settings

# Internet Fax transmission and reception

Interface

Ethernet (10BASE-T, 100BASE-TX)

Communication protocols

- Transmission

  SMTP, TCP/IP

- Reception

  POP3, TCP/IP

Transmission function

E-mail

E-mail format

Single/Multi-part, MIME Conversion

Attached file forms (transmission): TIFF-S (MH encoding)

Attached file forms (reception): TIFF-S/TIFF-F (MH/MR/MMR encoding)

Authentication method

SMTP-AUTH, POP before SMTP, A-POP

Original size

A4 (Length is up to 356 mm)

Scan line density

8 dots per mm × 3.85 line per mm (200 × 100 dpi)

8 dots per mm × 7.7 line per mm (200 × 200 dpi)

Destination machine specifications

- Communication protocols

  - Transmission

    SMTP, TCP/IP

  - Reception

    POP3, TCP/IP

- E-mail format

  - Format

    MIME, Base64

  - Content-Type

    Image/tiff

    Multipart/mixed (text/plain, Image/tiff (attached file forms))

- Data format

  - Profile

    TIFF-S

  - Encoding

    MH

  - Original size

    A4

  - Resolution (dpi)

    200 × 100, 200 × 200