ContentsPreviousNext
Settings

# Fax Transmission Setting Parameters

This section describes fax transmission setting parameters.

Immediate TX

Sets the machine to send a fax immediately when the original is scanned.

Default: [Off]

- Off

  Select this when using Memory Transmission.

- On

  Select this when using Immediate Transmission.

- Next Fax Only

  Select this when using Immediate Transmission for the next transmission only.

Resolution

Specifies the resolution to use for scanning originals.

The `“Photo”` resolution is not available for Internet Faxes. Faxes will be sent using `“Detail”` resolution if `“Photo”` resolution has been specified.

Default: [Standard]

- Standard

  Select this when the original is a printed or typewritten document with normal-sized characters.

- Detail

  Select this when the original is a document with small print.

- Photo

  Select this when the original contains images such as photographs or shaded drawings.

Density

Specifies the image density to use for scanning originals.

Default: [Normal]

- Light

- Normal

- Dark

Pause Time

Specifies the length of pause time when a pause is inserted between the digits of a fax number.

Default: 3 seconds

- 1 to 15 seconds

Auto Redial

Sets the machine to redial the fax destination automatically when the line is busy or a transmission error occurs, if the machine is in Memory Transmission mode. The number of redial attempts is preset to two or three times, depending on the [Country] setting under [Admin. Tools], in five-minute intervals.

Default: [On]

- Off

- On

Print Fax Header

Sets the machine to add a header to every fax you send. The header includes the current date and time, user fax name and fax number of the machine, job ID, and page information.

Default: [On]

- Off

- On

Original

Specifies the sides of the original (1 side or 2-sides) for scanning when using the ARDF in Memory Transmission mode.

When scanning 2-sides of original, specify the page and binding orientations according to those of the originals.

This setting only appears when the machine is in Memory Transmission mode for the Type 2 model.

Default: [1 Sided]

- 1 Sided

- 2 Sided Portrait: T to T

- 2 Sided Portrait: T to B

- 2 Sided Landscape: T to T

- 2 Sided Landscape: T to B