ContentsPreviousNext
Settings

# Basic Operation in Copier Mode

This section describes the basic procedure for making photocopies.

- The original in the ARDF or ADF takes precedence over the original on the exposure glass if you place originals both in the ARDF/ADF and on the exposure glass.

Press the [Copy] key.

Place the original on the exposure glass or in the ARDF/ADF.

If necessary, configure advanced photocopy settings.

To make multiple copies, enter the number of copies using the number keys.

Press the [Start] key.

If you are using the Type 2 model, depending on the machine's settings, `“Set Back Side”` appears on the screen when using the exposure glass.

- If you want to copy the back side of the original, proceed to the next step.

- If you want to end the job, press []. A copy will be output.

Turn over the original on the exposure glass, and then press the [Start] key.

A 2-sided copy will be output, and `“Set Front Side”` appears on the screen.

- If you want to copy the front side of the original again, turn over the original on the exposure glass, and then return to step 4.

- If you want to end the job, press [].

- The maximum number of copies is 99.

- You can change the paper tray for the current job by pressing the [][] keys. You can also select to change the paper tray automatically according to the paper size (A4 or Letter).

- You can select the paper tray for printing out copies in [Select Paper] under copy settings. If you set the machine to switch between tray 1 and 2 automatically depending on the paper size in this setting, you can also specify the tray the machine uses first in [Paper Tray Priority] under system settings.

- When making multiple copies of a multi-page document, you can select whether copies are output in collated sets, or in page batches in the [Sort] setting under copy settings.

- If [Manual 2 Sided Scan Mode], which is available only with the Type 2 model, is enabled, you can copy both sides of original with the exposure glass and make a 2-sided copy.

- If the time specified in [System Auto Reset Timer] under administrator settings passes without any operation while `“Set Back Side”` or `“Set Front Side”` is shown on the screen, the copying will finish automatically.

- To enable this function for the current job only, press [Dup/Comb] and select [Manual 2 Sided Scan Mode]. To use it as the machine's default setting, configure [Duplex/Combine] under copy settings.

- If a paper jam occurs, printing stops after the current page has been printed out. After the jammed paper is removed, printing restarts from the jammed page automatically.

- If a scanning jam occurs in the ARDF or ADF, copying is canceled immediately. In this case, copy the originals again starting from the jammed page.

- To place the original, see Placing Originals.

- To make reduced or enlarged copies, see Making Enlarged or Reduced Copies.

- To make combine or 2-sided copies, see Combining Pages and Making 2-sided Copies.

- To make copies of an ID card, see Copying Both Sides of an ID Card onto One Side of Paper.

- To make advanced scan settings, see Specifying Scan Settings.

- For details about [Select Paper] or [Sort], see Copy Settings.

- For details about [Paper Tray Priority], see System Settings.

- For details about [Manual 2 Sided Scan Mode], see Copy Settings.

- For details about [System Auto Reset Timer], see Administrator Settings.

- For details about how to remove the jammed paper, see Removing Printing Jams, or Removing Scanning Jams (Type 2 model) or Removing Scanning Jams (Type 1 model).

Related topics

Canceling a Copy