ContentsPreviousNext
Settings

# Configuring the Ethernet Speed

You can set the speed that the machine will use for Ethernet communications.

In most cases, this should be left on the default setting, [Auto Select]. This setting allows two interfaces to automatically determine the optimum speed when they are connected.

- Connection cannot be established if the selected Ethernet speed does not match your network's transmission speed.

- The use of this feature is recommended. To use it, select [Auto Select].

Router/HUB | Machine
--- | ---
[10Mbps Half Duplex] | [10Mbps Full Duplex] | [100Mbps Half Duplex] | [100Mbps Full Duplex] | [Auto Select]
10 Mbps half duplex |  | - | - | - |
10 Mbps full duplex | - |  | - | - | -
100 Mbps half duplex | - | - |  | - |
100 Mbps full duplex | - | - | - |  | -
auto-negotiation (auto selection) |  | - |  | - |

Press the [User Tools] key.

Press the [] [] keys to select [Network Settings], and then press the [OK] key.

If you are requested to enter a password, enter the password using the number keys, and then press the [OK] key.

Press the [][] keys to select [Ethernet], and then press the [OK] key.

Press the [][] keys to select [Set Ethernet Speed], and then press the [OK] key.

Press the [][] keys to select the Ethernet speed, and then press the [OK] key.

Press the [User Tools] key to return to the initial screen.

- You can press the [Escape] key to exit to the previous level of the menu tree.

- A password for accessing the [Admin. Tools] menu can be specified in [Admin. Tools Lock].

- For details about [Admin. Tools Lock], see Administrator Settings.