ContentsPreviousNext
Settings

# Configuring the Network Application Settings

Click the [Network Application] tab on the network settings page to configure the network application settings.

Scanner Send Setting
Item | Description
--- | ---
E-mail | Select to enable the Scan to E-mail feature.
Max. E-mail Size | Select the maximum size of scan files that can be attached to an e-mail message (1 to 5 MB, or no limit).
FTP | Select to enable the Scan to FTP feature.
Folder | Select to enable the Scan to Folder feature.

Network Print Setting
Item | Description
--- | ---
IPP | Select to enable network printing using Internet Print Protocol (via TCP port 631/80).
FTP | Select to enable network printing using an embedded FTP server in the machine (via TCP port 20/21).
RAW | Select to enable network raw printing.
Port No. | Enter the TCP port number to use for raw printing. The valid range is 1024 to 65535, except 53550 and 49999 (default is 9100).
LPR | Select to enable network printing using LPR/LPD (via TCP port 515).

mDNS Setting
Item | Description
--- | ---
mDNS | Select to enable Multicast DNS (via UDP port 5353). If disabled, the item below cannot be configured.
Printer Name | Enter the name of the machine. Can contain up to 32 characters.