C A S A F ile R ef .: D A T A -S H T .F R P 1 0/ 1 /9 2

PROFESSIONALQUALITYINCOMPUTER&ELECTRONICHARDWARE,COMPONENTS&MATERIALS

DATASHEET

Part Number:- UB-Mx-TL-TD-MAT(specialadder/suffix)

Date - 29th November,1997

P.O. Box 38-828 PETONE,Wellington Phone - (64-4)568 7277 )$;� � �

Ref - U-BOLTS.FRP

Arange of STANDARDM8U-Bolts (M6or M10sizes) can be designed and made at short notice to provide durable fixingfor Telecommunications Aerials, externally mounted Electrical,Electronicand other equipments.

Special Features Include:-

1) ISO Standard M6,M8and M10Threads (UNCand other thread forms can be made to order).

2) Wide range of Tube and Pipe sizes can be accommodated using flexibletoolingsystems.

3) "Dog-Point" lead, up to the thread, permits easy installationofNuts and washers etc..

4) Pre-packaged KITs includingall related nuts, washers etc. whichcan be suppliedto customer specifications

5) Manufactured in New Zealand using a combination of CNCmachiningand speciallydeveloped formtools.

6) Professional Quality at every level of design and manufacture.

Other Accessories (clamps and brackets) and alternative fastener types (including"J-Bolts"and "Hook-Bolts")can also be manufactured to customer drawing and specifications. Materials include Stainless, Aluminum, Brass, Copper, etc. Please enquire givingrelevant details.

Tube Sizes:-

(others available subject to toolingbeing made)

Threads:-

(other thread formsundertaken to special order)

Materials:-

(other alloys&materials subject to special order)

Fixing / Clearance Holes:-

(generallydepends upon requirements ofother parts)

Tensile Rating:-

Weight:- Size:- (Thread xLengthx Tube OD as below) Packaging:- (CASA’swelded Polyethylenebags and labels)

Provisional Specification Details:- (see physicaldetails on reverse ofthis data sheet)

UB- Mx- TL- TD- MAT

25.4mm OD(1.0 inch)

35~38mm OD(1.375~1.5")

48~54mm OD(1.875~2.125")

76mm OD(3.0 inch)

M6,M8,M10

(1/4",5/16",3/8"UNCetc.)

Stainless 304

(316, Aluminium, Steel etc.)

Diameter + 0.5mm

(recommended)

(to be calculated)

(type / model specific)

(type / model specific)

Loose or as required

Prefixto indicate"U-BOLT" Metricthread formwhere "x"= 6, 8 or 10mm. The overallthread lengthinmm includingthe "Dog-Point" Tube Diameter(nominal)inmillimeters Materialdesignator where "SS"= Stainless Steel, "AL"= Aluminumetc.

Please compose a

Part Number according to this system and use on yourofficialorder.

U-BOLTS(Stainless Steel etc.)