1 only Diaphram type compressor/vacuum pump - up to 20psi or 19" mercury - fitted with 3 anti-vibration feet and ancillary plumbing. Suitable for small air-brush, cleaning, vacuum holding etc.

Brand: Thomas Industries (USA)
http://www.thomaspumps.com/

Type: 264-3879 (IBM)
Model: 107CCD14 (nearest identifiable match)
Voltage: 230V 50/60Hz
Current: 0.7 Amps (50Hz)
Serial #: 0000187

FEATURES
• Oil-less operation
• Permanently lubricated bearings
• Stainless valves
• Die cast aluminum head, valve plate and diaphragm hold down plate
• Balanced for smooth, low vibration operation
• Long-life diaphragm
• Field service capability

Condition: NEW (un-used spares stock)

Assessed specification (based upon model number 107CCD14-230):

Pressure Flow Rate @ 0 pressure (SI / USCS) 15 l/min / 0.53 CFM Max.
Pressure Continuous (SI / USCS) 1,4 bar / 20 PSI Max.
Interim Pressure (SI / USCS) 1,4 bar / 20 PSI Max.
Pressure Restart (SI / USCS) 0 mbar / 0 PSI
Vacuum Flow Rate @ 0 vacuum (SI / USCS) 15 l/min / 0.53 CFM Max.
Vacuum Continuous (SI / USCS) 643.3 mbar / 19.0 IN.HG Max.
Interim Vacuum (SI / USCS) 643.3 mbar / 19.0 IN.HG Max.
Vacuum Restart (SI / USCS) 0 mbar / 0 IN.HG
Ambient Temperature, min. (SI / USCS) 10 °C / 50 °F
Ambient Temperature, max. (SI / USCS) 40 °C / 104 °F 
Motor Rating (SI / USCS) 90 W / 0.1 HP Speed 1700 rpm
Current Drawn 0.7 A Stroke (SI / USCS) 3.6 mm / 0.14 IN
Weight (SI / USCS) 2.3 kg / 5.1 lbs