
======================================================================
Fuji Xerox Network Scanner Utility2 Readme (Ver.5.8.5E) 
for Microsoft(R) Windows NT(R) 4.0
======================================================================

This document provides information about the utility on the following
items:

  1. Prerequisites
  2. Compatible models
  3. Installation
  4. Unique functions and cautions/limitations of the utility
  5. Cautions/Limitations on Accessibility
  6. Cautions/Limitations in the application of this scan driver 
  7. Revisions in this software version

* To use the scan driver, please select "FX Network Scan"
  as the TWAIN Data Source from the application.  

* This Readme explains the scan driver and Mailbox Viewer2.
  Unless otherwise stated, the information provided refers to
  the two features.

-----------------------------------------------
1. Prerequisites
-----------------------------------------------

* Required System Configuration

  This driver operates on a computer with an x86 processor,
  running Microsoft(R) Windows NT(R) 4.0 English version.  


  ** Available hard disk space of more than 5 MB for installation
     (When importing data from the scanner to your computer, you
     need to have a hard disk space double that of the data size.
     For example: A color A3 size document with 600dpi, need
     approximately two times 200MB,that is 400MB.)
  ** A display that is able to show more than 256 colors
  ** Windows NT 4.0 Service Pack 5 onwards
  ** Microsoft Internet Explorer 5.5 Service Pack2 onwards

* It is necessary to configure the TCP/IP settings in the scanner
  machine. 

* We recommend that you install at least 128MB of memory in
  the computer.

* We recommend that you use a display that is able to show more than
  65,000 colors.

----------------------------------
2. Compatible models
----------------------------------

Able Model-PRII
Document Centre 400/350/250
Document Centre 551/451 CP
Document Centre 706/606/506
Document Centre 285/235
Document Centre C400/C320
Document Centre 405/355
Document Centre C240
Document Centre 286/236
Document Centre C450/C360/C250
Document Centre 1100/900
DocuCentre C7550 I/C6550 I/C5540 I
ApeosPort C7550 I/C6550 I/C5540 I
DocuCentre 750 I/650 I
ApeosPort 750 I/650 I
Document Centre 336
DocuCentre 550 I/DocuCentre 450 I
ApeosPort 550 I/ApeosPort 450 I/ApeosPort 350 I
ApeosPort-II C4300/C3300/C2200
DocuCentre-II C4300/C3300/C2200
DocuCentre-II C3000
Fuji Xerox 4590/4110

* In the DocuCentre 551/451 CP series, "DocuCentre 550/450 CP" is displayed 
  as the Scanner Device Name.

* To use the network scanner function, some models will need
  options such as "Scanner Kit", "Function Extension Kit" and
  "Network Card". You may also need to expand your system
  memory. For details,please refer to the manual. 

-------------------------------------------
3. Installation
-------------------------------------------

* Note

  When using the Windows Explorer to perform the following operation,
  configure the setting to display all files in the Explorer beforehand.
 
 1) Select "Folder Options" from "Tools" of the Windows Explorer. The
    "Folder Options" window will be displayed.
 2) Click "View" > Select "Show hidden files and folders" under 
    "Hidden files and folders".
 3) Select the "OK" button to close the "Folder Options" window.

* Cancelling during installation / uninstallation

  The utility may not operate properly when the utility is already in the 
  process of installation and version update is selected, or when cancel 
  is selected during uninstallation. Re-install the software if cancel has
  been selected. 

* Installation and uninstallation can only be performed by users
  in the Administrators group.  

* Both the scan driver and Mailbox Viewer2 can be installed.

* Installing from CD-ROM

  Usually, when installing from the "CentreWare Utilities" CD-ROM,
  the CentreWare Utilities screen will appear automatically.  
  Select "Scan Driver" from this screen. Follow the instructions
  on the installer screen to proceed. If the installer is not activated
  either method automatically, choose(A) or (B) to install. 

* Installing from files downloaded via the Internet

  This section describes the installation when downloaded from
  our website via the Internet. Decompress the downloaded file
  before proceeding with the following operation. 

  Choose one of the following methods to install the driver.

 (A) Installing by using the "Add/Remove Programs" in Control Panel

 1) From the Start menu, select "Settings", followed by "Control
    Panel". Double-click the "Add/Remove Programs" icon.     
 2) Click the "Add New Programs" button in the "Add/Remove Programs"
    dialog box and click the "CD or Floppy" button. Click the "Next"
    button to proceed. A "Run Installation Program" dialog box will
    be displayed.
 3) Click the "Browse" button and select the setup.exe file on the
    Browse screen. (The setup.exe is in the decompressed Disk 1 folder.)
    Click the "Open" button and then click the "Finish" button.
    If you are using the "CentreWare Utilities" CD-ROM, the program 
    can be found in the "Scan\Setup\Disk 1" directory of the CD-ROM drive.
 4) Follow the instructions on the Installation screen to proceed.
    Specify the directory and the program folder name for
    installation.
 5) Follow the instructions on the screen to proceed. 
    Selecting the "Complete" button ends the installation.

 (B) Installing by executing SETUP.EXE

 1) Select "Run" from the Start menu.
 2) Enter the directory for the Disk 1 folder and select Setup.exe.  
    For example, if the CD-ROM drive is E, 
    enter "E:\example\Disk1\Setup". 
 3) Follow the instructions on the Installation screen to proceed.
    Specify the directory and the program folder name for
    installation.
 4) Follow the instructions on the screen to proceed and
    insert the second disk. When all necessary files are
    copied, the "Complete" button will be displayed.
    Selecting the "Complete" button ends the installation.

------------------------------------------------------------
4. Unique functions and cautions/limitations of the utility 
------------------------------------------------------------

About this Utility

This scan driver is used to import scanned images stored in the
mailbox of the scanner to TWAIN interface-compatible applications
operating on Windows NT4.0 environment.

Select "FX Network Scan" as the TWAIN data source.
The Mailbox Viewer2 is a mailbox utility that accesses the mailbox
periodically and sends a notification when a new document is received.
As this Utility is commonly used for multiple models, some functions 
or settings will not be displayed depending on the models used.
For details on the functions of the utility, refer to the on-line
Help dialog box.

* For customers who have used the Network Scanner Utility
  
  When you install the Network Scanner Utility2, the Network Scanner
  Utility that you have been using will be deleted. As "FX Network
  Scan Driver" will become "FX Network Scan" in the TWAIN data
  source, select "FX Network Scan".
  This utility includes features of the drivers and Mailbox Viewer
  thus far.

* Using software with Personal Firewall function (including Internet
  Connection Firewall/Windows Firewall)

  When this utility is used on a computer installed with Personal
  Firewall, the scanner device may not be connected. 
  Set the settings such that the port to be used by the utility is 
  not blocked.
  Please see the following steps for example.  
  However, with Firewall set up, it may take a longer time to
  connect to the scanner device and import files even if the
  following settings are specified.

  ** Norton Personal Firewall 2003 / 2004

   1) Activate Norton Personal Firewall from the Start menu. 
   2) Select "Personal Firewall" from the "Status & Settings" 
      screen and click the "Configure" button. 
   3) Go to the "Program Control" tab at the settings screen. 
   4) Click the "Add..." button at "Manual Program Control". 
   5) Select \Program Files\Fuji Xerox\Network Scan
      \FxsUtl12.exe and click the "Open" button. 
   6) Select "Permit" at the "Program Control" screen and click the
     "OK" button. 
   7) Select "General" at the "Choose Application Category" screen 
      and click the "OK" button. 
   8) Perform Steps 4 to 7 for \windows\System\fxsslm12.exe also 
      to authorize program control.
   9) If you are using the TWAIN driver, perform the same steps 
      for the .exe file applications to authorize program control. 
      For example: Specify the following exe file for DocuWorks. 
      \Program Files\Fuji Xerox\DocuWorks\bin\dwdesk.exe

  This utility may not function properly when the "TCP/IP 
  Filtering" feature of the Internet Protocol (TCP/IP) provided by 
  Windows is enabled.

* This utility may not operate if there are multiple network cards
  connected to the Computer.

* About the display for scanner device list

  ** If the display for scanner device list is slow, perform 
     steps 1) to 5) below.
  ** If there is a router between the scanner device and client  
     computer, perform the steps 1) to 4) below.
  ** If you want to change the scanner device names displayed  
     on the scanner device list, perform the steps 1) to 4) below.

  1) Activate the scan driver (Mailbox Viewer2).
  2) Click the "Options" button on the Mailbox Viewer2 dialog that
     displays a list of scanners.
  3) Select the "Display registered scanners" check box in Scanner
     Registration.
  4) Select the "Add" button and enter the IP address and an optional
     scanner name of the scanner to be used.
  5) Uncheck the "Seach local network scanners" check box.
 
  When the IP address of a device incompatible to this utility is 
  registered or when a scanner is not powered up, the device will 
  still be displayed.  However, if this scanner device is selected, 
  an error message stating, "The selected scanner device does 
  not exist" will appear.  
  When this happens, please make sure that the IP address is 
  correct and the scanner device is powered up.  
  If the registered device exists on the local network and "Search 
  local network scanners" is selected, the registered device name 
  will appear.  

* Document deletion timing

  When a Computer imports data from a scanner, the document
  stored in the Mailbox will be deleted once the last page of the
  document has been imported. (If the Mailbox setting is set such
  that the document will not be deleted after import, it will not be 
  deleted even after it has been imported.)

  It is possible that the document might be deleted before it
  is imported, if the importing process is met with the following
  interruptions at the Computer: 

  ** an error occurs during the process of compression and
     uncompression at the Computer
  ** the Cancel button of the utility is pressed and the
     importing process is cancelled  
  ** the Computer is rebooted

  When this happens, the document cannot be imported again.

* When Scanner Driver and Mailbox Viewer2 is used concurrently

  ** Scanner driver and Mailbox Viewer2 cannot be used concurrently 
     on the same computer. Also, mulitple scanner drivers and Mailbox 
     Viewer2 cannot be used at the same time.

* Simultaneous connection to scanner device

  This model has the following limitations.

  1) Data from the same scanner device cannot be imported to 
     multiple computers with this utility. However, the information
     on the list of files can be displayed. 
  2) Files cannot be imported from the scanner device during fax 
     transmission. However, the information on the list of files can be 
     displayed from the utility. 

  In any case, you have to import again after the job processing is completed.

* When a decoding error occurs while a FAX document is being imported

  When a decoding error occurs while a FAX document is being imported,
  that particular page might not be correctly displayed on the screen.

* About pages when transmission is disconnected during importing

  If transmission between the multi-function machine is disconnected
  when importing a document that is stored in the mailbox,
  the imported page may not be displayed correctly.

* Importing multiple documents
 
  When importing multiple documents stored in the mailbox,
  communication with the machine will be cut off temporarily while
  importing each document.
  The importing process may be terminated if the scanner is being
  used by other computers during this process.

* When image importing is in progress, select the space key or the
  Enter key to cancel.

* Usually when the Cancel button is selected, it becomes suppressed.
  Display GUI before selecting Cancel. 
  However, depending on the progress of the cancellation, GUI may not
  be displayed.

* The following characters cannot be used as the path name for
  "Temporary Save in", "Save in" and "Folder Naming".
  
   \ / : * ? " < > |

* Text Used for File Name or Location

  If text which cannot be displayed using Windows are included in the
  file name or location, they will not be displayed correctly in the 
  File Name or Location of the network scanner dialog box.
  Moreover, if File Name or Location is selected at Naming of the
  Import Settings dialog box, text that cannot be displayed correctly
  will be changed to "_". If the text cannot be changed, the file name and
  location will not be added to the folder.

* If the mailbox is configured not to delete data after importing,
  the Mailbox Viewer2 will not be able to import the same data again
  after importing it once. The imported data will be saved in the specified
  location in "Save in" and if the data is moved, it can be imported again.

* When the Mailbox cannot be opened

  The document stored in the scanner may be corrupted if an error
  message "Invalid password" always appear and the contents of the
  Mailbox cannot be displayed even though the Mailbox number and
  password are correctly entered. 
  When this happens, delete the document data that is stored in the
  Mailbox.

* When the file space specified at "Temporary Save in" and "Save in"
  is insufficient
  
  If there is insufficient file space in the specified location at
  "Temporary Save in" and "Save in", the documents cannot be imported
  correctly and may be destroyed. 
  Specify a drive with enough free space.

* Port Conflicts

  If the port to be used in this utility is being used by another
  application or service, the following message will be displayed:

    "Network Scanner Utility2 is not available as the port conflicts
     with another application or service.
     End the application or service first, and then retry."

  In this case, you must end the application or service using the port.
  After that, re-execute this utility.
  Please also refer to the following section on "*** Software 
  programs and services that cannot be run concurrently".  

* Software programs and services that cannot be run concurrently

  If the following software programs and services are running on 
  the same computer as this utility, this utility will not run properly.
  Do not run the following software programs and services concurrently 
  with this utility. 

  <Software programs that cannot be run concurrently>
  Fuji Xerox (Ltd) CentreWare Mailbox Agent
  Fuji Xerox (Ltd) Document Director
  Muratec Sales (Ltd) OfficeBridge

* Precautions when using the Internet Explorer (IE3.0/4.0)

  When using the Internet Explorer as a browser, priority will be
  given to TCP/IP access for Dial-Up Network connection if the
  "Connect to the Internet as needed" check box in the Connection tab
  of the Internet properties dialog box is checked.
  If the check box is checked, the Dial-Up connection window will be
  opened each time the scan driver is activated.  At this
  point, the scan driver will be activated if the Dial-Up
  Connection window is cancelled. 

-------------------------------------------------------------
5. Cautions/Limitations on Accessibility
-------------------------------------------------------------

* Limitations due to software specification

  ** Only the first four characters of a password are used,
     even if more are entered. 
  ** The same label can be read twice.
  ** Phrases that are not displayed can also be read.

* Other Limitations

  ** The bold frame indicating the correct focus may not be displayed 
     for  the control with the correct focus. The read software will
     still perform reading. 
  ** The focus may be shifted for controls that cannot be changed 
     when  using a TAB key. 
  ** The default settings of the "Animation Display When Importing" 
     for scan driver depends on whether the screen reader is 
     activated when installing this utility. 
     The animation will not be displayed if the screen reader is 
     activated and vice versa.
     However, as the diagnosis may not be correct depending on the
     environment used, you can change the animation display settings
     manually at the "Display Animation When Importing" at the 
     scan driver settings screen if desired.

--------------------------------------------------------------
6. Cautions/Limitations in the application of this scan driver
--------------------------------------------------------------

This section describes the cautions and limitations for individual 
applications that are identified.  

* All applications
  ** Memory error or freezing/hanging of application may occur when 
     importing huge images. 
     As the imported document may be deleted, check the 
     specification of the application before using and import an image 
     that does not exceed the permitted value. 
  ** When document scanned in pseudo-grayscale is imported, spots may 
     appear on the image.  
  ** For applications that do not support multi-page document, only the 
     first page will be imported even though multiple pages of the scanned 
     document are imported. 
     In this case, open the "Settings" dialog box from the "Settings" button 
     of the scan driver and then select "By page" for the "Display Mode".
     As the document information will be divided and displayed one page
     at a time with this setting, import the images of these divided
     pages one page at a time.
     Only the first page will be displayed.
  ** For applications with gradient correction function, the 
     orientation of the imported document will be rotated and the 
     display may be  tilted. This problem can be avoided if you do not 
     select the gradient correction in the application. Read the 
     application manual on the  method of setting gradient correction.
  ** Depending on the application, there are limitations on the display
     of multi-page TIFF file created by Mailbox Viewer2. 
     This includes one of the following.

     1) Cannot be displayed or only the first page is displayed.
     2) All pages or only the first page of the uncompressed color and
        grayscale multi-page tiff file are displayed.  
     3) Documents with color and black/white pages or mixed size multi-
        page Tiff file is not displayed. 
     4) Only the first page of a multi-page Tiff file consisting of only
        black/white pages is displayed.

* Fuji Xerox Co., Ltd.    DocuWorks Ver. 3.1.6/DocuWorks Ver. 4.0.5
                           / DocuWorks Ver. 5.0

  When images exceeding the size limit specified in DocuWorks are 
  scanned, an error will occur.  For details, please refer to the 
  DocuWorks Help. 

  When scanning a long document, the width of the document will
  determine the standard paper size to be used. Thus the long
  document will be divided equally based on the standard paper size
  and become a multi-page document.

  If "Fit to Standard Size Paper" is selected, the unintended paper
  size may be selected. When this happens, change the settings at
  DocuWorks Desk according to your needs.
  
  For example, when the scanner reads an A4 size document as Letter.
  In this case, configure the following settings at the DocuWorks
  Desk.

  1) Select Option... from File of the DocuWorks Desk.
  2) Click the "Scan and Import" tab.
  3) Check the box next to "Fit to Imported Image".
 
  If the paper size of an imported document is greater than A3 size,
  configure the following settings at the DocuWorks Desk to reduce it
  to A3 size.
  
  1) Select Option... from File of the DocuWorks Desk.
  2) Click the "Scan and Import" tab.
  3) Check the box next to "If scanned image exceeds A3 size, fit it
     into A3.".  

  For DocuWorks Ver. 3.1.6, if the first page of an uncompressed
  multi-page TIFF file with color and black/white pages imported by
  Mailbox Viewer2 is a color page, the file will not be displayed.

  For DocuWorks Ver. 3.1.6, all pages of a multi-page TIFF file
  imported by Mailbox Viewer2 will be standardized and displayed
  in the size of the first page.

  In DocuWorks V5.0, the name attached to the documents by the 
  scanner device can be used as the name for DocuWorks document.   
  Follow the steps below to use the file name. 

  Please refer to the manual to check whether file names can be
  attached in your scanner device. Please use the latest version
  of the scanner driver. 

  To inherit the document name, follow the procedure below: 

   1) File -> DocuWorks Desk Options
   2) Select "Save Scanned Document" 
   3) Select "Document name given during scanning will be used as 
      the scanned document name"

  When this driver is associated with DocuWorks 5.0 and the scanned 
  image is imported from the mailbox to DocuWorks Desk, scanning 
  may fail with a message stating "TWAIN Communication Error" appears.  
  When this happens, you can install Network Scanner Utility2 Ver. 3.0.4 
  or later to rectify the problem.   
  In the previous driver version, problem will occur when the document 
  name including path length exceeds 126 bytes. In DocuWorks 5.0, the 
  same problem is expected if the hierarchy of the folder path exists 
  deep down the directory during standard installation.  

  If document with width or length exceeding 500mm is scanned, the 
  area that has exceeded 500mm will not be displayed.  For sizes such 
  as A0, if both the width and height of the original document exceed 
  500mm, the dimension that will be displayed is 500mm x 500mm.  
  If the size of the original document exceeds the dimension of A3 size,
  follow the steps below.  

  1) File (F)  > DocuWorks Desk Options (O)
  2) Select "Scan and Import" tab. 
  3) Select "If scanned image exceeds A3 size, fit into A3 (M)". 

* Adobe Systems, Inc. Adobe(R) Acrobat 4.0/Adobe(R) Acrobat 5.0

  If Cancel is selected during the importing process from the scan
  driver, an error message will appear. However, you can still
  continue to use the scan driver.
  
  When importing cannot be performed due to insufficient virtual
  memory, you can resolve this problem by changing to an available
  drive where the environmental variable TEMP has sufficient disk
  space.

  When importing to Acrobat cannot be performed due to the
  limitations of the image size, an error message stating, "Could
  not complete the acquisition because of a problem with the device."
  will be displayed.

* Adobe Systems, Inc.  Adobe(R) Acrobat 6.0

  Multiple pages (documents) cannot be imported in a batch.  
  Open the dialog box using the "Settings" button in the scan 
  driver,then select "By page" for "Display Mode" and import one 
  page at a time.

  [Save Password] feature is enabled automatically.  
  To change the scanner device or the mailbox, press 
  the [Change Scanner] button to go to the screen which shows
  a list of scanner device.  

  When a document is imported using Acrobat 6.0, an asterisk (*) 
  will be attached at the extreme left of the imported page and may 
  be displayed in the document list.
  When this image is displayed using Acrobat, the image at the lower 
  end may be missing. If this happens, open the file that is 
  imported via Mailbox Viewer2 using Acrobat.
  If there are unwanted pages after importing all the pages, use the 
  "Delete" button to delete all of them.

* Adobe Systems, Inc.     Adobe Photoshop 5.5/Adobe Photoshop 6.0
                             /Adobe Photoshop 7.0/Adobe Photoshop CS

  According to Photoshop specifications, a long document of maximum
  30000 pixels x 30000 lines can be read by the application.  When
  this limit is exceeded, an error message will appear if you try to
  import the document and after which, the scan driver dialog box
  cannot be closed.  When this happens, terminate Photoshop by
  pressing Ctr+Alt+Del.
  
  Depending on the memory size of the Computer, an error message
  stating, "Network connection failed" may appear after "Select
  TWAIN_32 Source..." is executed. When this happens, reduce the
  memory size by approximately 50% at Memory & Image Cache... of
  Preferences from File (for Ver. 5.5) or Edit (for Ver. 6.0).

* Microsoft Corporation  Word 2000/Word 2002 / Word 2003
* Microsoft Corporation  Excel 2000/Excel 2002 / Excel 2003
* Microsoft Corporation  PowerPoint 2000/PowerPoint 2002

  Missing pages or document loss may occur when importing By File,
  therefore, it is necessary to use By Page.
  
  For Word 2000/Excel 2000/PowerPoint 2000, if the data to be
  imported is too large and the resolution is too high, it may
  not be imported. Reduce the size of the data or the
  resolution.

* Microsoft Corporation  PhotoDraw 2000

  Documents exceeding 3968 lines cannot be read by the application.
  Thus documents of the following sizes and resolutions will be
  displayed as blank sheets of paper:
  
  A4/Ledger and above with 300dpi
  B5/Letter and above with 400dpi
  All sizes with 600dpi
  
  However, the scanned images still remain in the mailbox.
  You can use other applications or the Mailbox Viewer2 to import the
  scanned images. After importing, if the scanned images still remain
  in the mailbox, delete them by clicking the Delete button on the
  dialog box. 
  For iFAX documents, the first page will be displayed as a blank
  sheet if the mail header of the first page is a 600dpi-product. 

  When importing multi-page document by file, configure the "Method"
  to "Your Scanner Software". 

  You can find "Method" in the following location:
  Select "Scan Picture" from File to display the "Scan" screen.
  You will find "Method" on the screen.

* Microsoft Corporation  PhotoEditor 3.01/PhotoEditor 3.0.2.3
  
  Documents containing both B/W and color pages cannot be scanned.  

  Mixed size documents cannot be scanned.  

  If the data to be scanned is too large and the resolution is too
  high, it may not be scanned. Reduce the size of the data or the
  resolution. iFAX documents will be displayed as blank sheets as the
  mail header for first page is 600dpi. However, if you import the
  documents by page, you will be able to import from the second page
  onwards. 

* Microsoft Corporation    Picture It! 2/Picture It! 2000

  Document exceeding 3968 lines cannot be read by the application.
  
  If the data to be scanned is too large and the resolution is too
  high, it may not be scanned. Depending on the model, iFax document 
  cannot be imported as the first page of mail header is 600dpi. 
  However, if you import the documents by page, you will be able to
  import from the second page onwards. 

  When importing a document of multiple pages that was scanned using
  the Automatic Document Feeder, if the size of each page and the
  resolution are different,subsequent pages after the first page may
  not be imported correctly.When this happens, select "By page"
  and import one page at a time.
  
  If Cancel is selected during the importing process from the scan
  driver, an error message will appear. However, you can still
  continue to use the scan driver.

  For Picture It! 2, the "Smart Task Scan" of "Scanning Method" is
  not supported.

  For Picture It! 2000, if the "Smart Task Scan" of "Scanning Method"
  is selected, an error message will appear when you quit the scan
  driver but there will be no problem the next time you use it.

* ScanSoft, Inc. OmniPage(R) Pro 10/OmniPage(R) Pro 11
  
  For OmniPage(R) Pro 10, select "Yes" for "Show TWAIN settings
  before scan" of the "TWAIN Scanner Settings".
  
  You can find "TWAIN Scanner Settings" in the following location:
  
  Display the Control Panel screen on the windows. Click "Caere Scan
  Manager 5.0" to display the "Caere Scan Manager 5.0" screen.
  Select "TWAIN SCANNER" to display the "TWAIN SCANNER 
  Properties" screen. You will be able to find "TWAIN Scanner Settings".
  
  Do not select "AutoOCR" for OmniPage(R) Pro 10.
  
  For OmniPage(R) Pro 11, if the data to be imported is too large and
  the resolution is too high, it may not be imported. Reduce the size
  of the data or the resolution.  
  
  For OmniPage(R) Pro 10 and OmniPage(R) Pro 11, the documents
  cannot be imported by file. Import the documents by page.

* ScanSoft, Inc. Pagis PRO 97/Pagis PRO 3.0
  
  If Cancel is selected during the importing process from the scan
  driver, an error message will appear. However, you can still
  continue to use the scan driver.

  For Pagis PRO 97, configure the correct settings for "Document
  Contents" and "Color depth" depending on the type of document
  (color/grayscale/black and white) before importing files. In the
  event that you have imported the scanned images with incorrect
  settings, they will still be stored in the mailbox. Configure the
  correct settings and import again. After importing, if the scanned
  images still remain in the mailbox, delete them by clicking the
  Delete button on the dialog box.
  
  For Pagis PRO 97, if the data to be imported is too large and
  the resolution is too high, it may not be imported. Reduce the size
  of the data or the resolution.  
  
  For Pagis PRO 97, if you quit the scan driver, an error message
  will appear but there will be no problem the next time you use it.
  
  For Pagis PRO 97, the documents cannot be imported by file. Import
  the documents by page.

  For Pagis PRO 3.0, for documents with color and black/white pages,
  the display orientation for color and black/white pages may be
  different. Uncheck the "Auto Orient" selection to prevent this
  problem from occurring. 
  You can find "Auto Orient" in the following location:
  
  Click the scanner icon on Pagis PRO 3.0 and the "Pagis Scan Tool-
  Scanner" screen will be displayed. Select "Properties..." and the
  "Properties-Any Document" screen will appear. You will find "Auto
  Orient" on the screen.

* ScanSoft, Inc. TextBridge PRO 98/TextBridge PRO 9.0/
                     TextBridge PRO Millennium
  
  The limit for a long document is about 20000 lines. 
  
  Set the "Scanner Settings" to "Scanner's TWAIN dialog box".
  When "TextBridge Settings" is set, importing can be done normally
  but the scan driver might not be able to quit normally.
  
  If Cancel is selected during the importing process from the scan
  driver, an error message will appear.

  TextBridge PRO 98 does not support color and grayscale. In the
  event that you have imported the scanned images with incorrect
  settings, they will still be stored in the mailbox. You can use
  other applications or the Mailbox Viewer2 to import the scanned
  images. After importing, if the scanned images still remain in the
  mailbox, delete them by clicking the Delete button on the dialog
  box.

  For TextBridge PRO 98, if you click the TextBridge PRO 98 window
  using a mouse when the scan driver screen is displayed, the
  scan driver screen will be hidden at the back of the screen. If
  this happens, bring it to the front.
  
  For TextBridge PRO 98, if the data to be imported is too large and
  the resolution is too high, it may not be imported. Reduce the size
  of data or lower the resolution.
 
  For TextBridge PRO 9.0, ServicePack1 is required in order to
  activate the scan driver.                         
                        
  For TextBridge PRO 9.0/TextBridge PRO Millennium, the resolution of
  the image from the scan driver will be changed by the application.

* ScanSoft, Inc. PaperPort 10

  To display images, use PaperPort 10 to open the file read by Mailbox
  Viewer 2.
  Do not use the TWAIN function. 

* ScanSoft, Inc. PaperPort DELUXE 8.0
* Visioneer, Inc. PaperPort DELUXE 4.0/PaperPort DELUXE 7.0

  The limit for a long document is about 20000 lines.

  Rough images may be displayed for black/white images. When this
  happens, go to "Display" and check "Grayscale" for a smooth image.

  When importing mixed size documents, all pages are assumed to
  have the same size and resolution as the first page.  Thus
  subsequent pages that are different from the first page may not be
  displayed correctly.
  When this happens, select "By page" and import one page at a time.
  
  The limit for a long document is about 20000 lines.  When this is
  exceeded, an error message from Imaging will be displayed.

* WANG Laboratories, Inc.  Imaging for Windows Professional Edition
                           Release 1.1

  Importing using Imaging for Windows Professional Edition Release 1.1
  will be cancelled if the following have been imported:

  When a document with color and black/white pages has been imported
  When a mixed size document has been imported
  When a document with different resolutions has been imported
  When a color document and a black/white document have been imported
  at the same time
  When documents of different sizes have been imported at the same
  time
  When documents of different resolutions have been imported at the
  same time 

  When this happens, pages that have been imported correctly will be
  stored in the application.
  Follow the procedure below to continue scanning.

  1) Re-display the list of documents in the computer where importing
     was conducted.
  2) Select the "Settings" button to open the Settings dialog box.
  3) Configure the "Display Mode" to "By page".
  4) Import the remaining pages one page at a time.

  When importing mixed size documents, all pages are assumed to
  have the same size and resolution as the first page.  Thus
  subsequent pages that are different from the first page may not be
  displayed correctly.
  When this happens, select "By page" and import one page at a time.
  
  The limit for a long document is about 20000 lines.  When this is
  exceeded, an error message from Imaging will be displayed.

--------------------------------------------------
7. Revisions in this software version
--------------------------------------------------

Ver. 3.0.2E
Added the compatible machine types for monochrome multi-functional
machines in the market. (Refer to the list below.)

If the network scanner utility for monochrome multi-functional
machine has already been installed on the Computer, it will be
deleted and replaced with network scanner utility2 when you
install the latter.
<Added Machine Types>
Adobe Model-PRII
Document Centre 400/350/250
Document Centre 550/450 CP
Document Centre 706/606/506
Document Centre 235
Document Centre 285

Resolved the time-out problem which occurred when logging in
to NetWare during importing.

Ver. 3.0.4E
Rectified the problems in the help file.
Resolved the problem where the file name created by the scanner device
cannot be changed to the DocuWorks file name using DocuWorks V5.0.

Ver. 3.0.5E
Resolved the problem where the files in Disk 1 cannot be stored
completely in a floppy disk. 

Ver. 3.3.0E
Added support for Document Centre 355/405. 
Resolved the problem where documents have been deleted when importing
from Imaging.
(Please refer to Cautions/Limitations in the application of this scan driver)

Ver. 3.4.2E
Added support for Search local network scanners which allows you to
select whether to enable or disable the search for local network
scanners.
Resolved the problem where TIFF files are detected during processing
from the software which converts the created TIFF file when Save in
is specified in the Mailbox Viewer2.
Resolved the problem where the scroll bar was not enabled when a
great number of the scanner devices have been displayed.

Ver. 3.5.0E
Resolved the problem where documents cannot be imported from
FireWorks.

Ver. 3.5.1E
Increased the limit of scanner registration to a maximum of 50
entries at the Change Scanners dialog box.
Resolved the problem where the same name has been used to register
the device.
Resolved the problem where importing cannot be performed when "Folder
Naming" has been selected and an error message stating, "Problem
occurred during compression," is displayed.
Resolved the problem where an application error occurred when
importing a specific fax document that is received.
Resolved the problem where importing cannot be performed when the
allocated network drive has been specified in Temporary Save in.

Ver. 3.6.0E
Added support for high contrast settings (black and white) for
display.
Resolved the problem where the play button on the WAVE file
selection screen of the Mailbox Viewer2 cannot be selected using
the Tab key.
Added support to the scan driver which allows one to select
whether to display the animation during importing.

Ver. 3.6.1E
If transmission between the multi-function machine is disconnected
when importing a document that is stored in the mailbox, parts of
the document which have been imported to the computer before
disconnection can be retrieved.

Ver. 3.6.2E
An error message can now be displayed when there is a conflict with
ports.

Ver. 3.6.3E
Improved the performance of importing files with many pages.

Ver. 3.7.0E
Added support for Document Centre C240.

Ver. 3.7.1E
Added support to display error messages when the ports are
conflicting.
Improved the performance when scanning large volume documents.
Enabled the creation of image data for the successfully decoded data 
even if a decoding error has occurred while importing with 
Mailbox Viewer2 or scan driver.
Resolved the problem where uninstallation cannot be performed when
double-byte characters are included in the login name.

Ver. 4.0.0E
The selections for functions that are not supported by the model that 
you are using will be disabled. For models that support additional 
options, functions that are provided by these options will be enabled 
even if these options are not installed.  
The scan driver will always scan one page at a time for multi-page
scanning in Acrobat 6.0. 

Ver. 4.1.2E
Improved the scan performance when large amount of documents
are stored in the mailbox. 

Ver. 4.2.0E
Added support for Document Centre 286/236.  

Ver. 4.3.0E
Restricted the use of port for external transmission and 
improved the convenience when used in an environment  
configured with Personal Firewall.

Ver. 5.1.2E
Added support for Document Centre C450/C360/C250.
When "File Name or Location" is selected, whether the priority
is given to file name or location depends on the file type. 
Resolved the occasional occurrence of PC freezing during installation.

Ver. 5.1.5E
Added support for Document Centre 1100/900.

Ver. 5.2.1E
Changed the path from Start menu to "Mailbox Viewer2".
Made it possible to display "Readme" from the Start menu.

Ver. 5.2.2E
Changed the operation for continuous import from Acrobat 6.0.

Ver. 5.2.5E
Resolved the problem of part of the text used in the path for user 
name, "Save in", "Temporary Save in".  

Ver. 5.3.1E
It is no longer necessary to restart Windows after installation.
Software such as ARCServe2000 SP3 and Service for UNIX can 
now coexist together.  

Ver. 5.3.5E
Added support for DocuCentre C6550 I/C5540 I series.
Added support for ApeosPort C6550 I/C5540 I series.

Ver.5.4.3E
The layout of the [Import] button and the [Save in] input box on
the operation screen of Mailbox Viewer2 has been changed.
"Save in" can now be specified using the UNC path.
When importing multiple-page document using [By file] setting,
only pages that have not been imported will be imported.  
For PC operating with multiple processors (including
hyper-threading), the problem (*) of Network Scanner Utility2
hang-up has been resolved. 
(*) When using CentreWare Flow Services, polling to the mailbox
of device is stopped.

Ver.5.5.0E
Resolved the problems related to operations of stopping importing 
by TWAIN scan driver.
Set up restriction on the number of password entries.
Indicated version in title bar.

Ver.5.5.1E
Added support for DocuCentre 750 I/650 I series.
Added support for ApeosPort 750 I/650 I series.

Ver.5.5.4E
Added support for Document Centre 336.

Ver.5.5.5E
Added support for DocuCentre 550 I/DocuCentre 450 I series.
Added support for ApeosPort 550 I/ApeosPort 450 I/ApeosPort 350 I series.

Ver.5.5.9E
Added support for DocuCentre C7550 I series.
Added support for ApeosPort C7550 I series.

Ver.5.6.2E
Added support for DocuCentre-II C4300/C3300/C2200 series.
Added support for ApeosPort-II C4300/C3300/C2200 series.

Ver.5.6.5E
Added support for DocuCentre-II C3000 series.

Ver.5.7.5E
Added support for Fuji Xerox 4590/4110 series.

Ver.5.8.1E

Ver.5.8.3E

Ver.5.8.5E

Ver.5.9.0E

* Checking version information
  On each dialog of the Utility, you can click the icon on the
  top left to display the pull-down menu and then select "About" to
  check the information.


Adobe, Acrobat and Adobe Photoshop are registered trademarks or
trademarks of Adobe Systems Incorporated and its subsidiaries in
each country.

Intel, i486 and Pentium are registered trademark of Intel
Corporation of America.

Microsoft, Windows and Windows Server are
registered trademarks of Microsoft Corporation of America.

Xerox, Able and DocuWorks are registered trademarks of Fuji Xerox.

Citrix, MetaFrame, ICA are the trademarks or registered trade
marks of Citrix Systems, Inc. (America) and other countries.

All other product/company names are registered trademarks or
trademarks of the respective companies.
