ContentsPreviousNext
Settings

# Unsupported Types of Paper

Avoid using the following paper as they are not supported by this machine.

- Paper meant for an ink-jet printer

- Bent, folded, or creased paper

- Curled or twisted paper

- Torn paper

- Wrinkled paper

- Damp paper

- Dirty or damaged paper

- Paper that is dry enough to emit static electricity

- Paper that has already been printed onto, except a preprinted letterhead.

  Malfunctions are especially likely when using paper printed on by other than a laser printer (e.g. monochrome and color copiers, ink-jet printers, etc.)

- Special paper, such as thermal paper, aluminum foil, carbon paper and conductive paper

- Paper that is heavier or lighter than the specified limitations

- Paper with windows, holes, perforations, cutouts, or embossing

- Adhesive label paper on which the adhesive under-layer or base paper is exposed

- Paper with clips or staples

- Do not use ink-jet printer paper because it may stick to the fusing unit and cause a paper jam.

- Do not use paper that has already been printed onto by other printers.

- When loading paper, take care not to touch the surface of the paper.

- Even supported types of paper may cause paper jams or malfunctions if the paper is not in good condition.