ContentsPreviousNext
Settings

# Configuring the storing conditions

To specify the storing conditions for received faxes, configure the machine as follows:

1. Select [Print] for [Reception File Setting] under fax feature settings to store received faxes in memory for printing.

2. Configure the print setting for faxes stored in memory in [Print Received File] under fax feature settings.

   - [On]: Automatically print out the received faxes and delete from memory.

   - [Off]: Store the received faxes in memory for later manual printing.

- When the fax is successfully printed out, it will be deleted from memory.

- If the machine is unable to print out a fax due to machine errors such as an empty paper tray or a paper jam, the fax will remain in memory and the Fax Received indicator will flash. The remaining pages will start printing as soon as the problem is resolved.

- For details about the control panel settings, see Fax Feature Settings.

- To manually print out received faxes stored in memory, see Printing Out Faxes Stored in Memory.