ContentsPreviousNext
Settings

# Specifying the scan destination from an LDAP server

This section describes how to select a destination registered on the LDAP server.

- To search for a destination from an LDAP server, the LDAP server must be registered in advance, and [LDAP Search] must be enabled under the LDAP server settings.

- You can search Scan to E-mail destinations from the LDAP server (not Scan to FTP or Scan to Folder destinations).

Press the [Scanner] key.

Press the [Address Book] key.

Press the [][] keys to select [Search LDAP], and then press the [OK] key.

Press the [][] keys to select [Start LDAP Search], and then press the [OK] key.

A list of destinations that match the search conditions appears on the display (up to 50).

Press the [][] keys to scroll through the search result, and then press [] to select the desired destination.

You can select multiple destinations. A check mark will appear for the selected destinations. To deselect a destination, press [] again.

- The search result will contain destinations that match the predefined search conditions.

- To send scanned files to the destinations specified from the LDAP server, you must select the file format after pressing the [Start] key to execute scanning. The file format depends on the [Scanning Mode] setting under scanner settings:

  - When in black-and-white scanning mode: TIFF or PDF

  - When in color or gray scale scanning mode: JPEG or PDF

- The scanned files to the destinations specified from the LDAP server will be created with the machine's current scan settings. If necessary, configure the scan settings before executing scanning.

- If a record that has been found contains multiple destinations, the first of those destinations will be used.

- For details about registering LDAP servers, see Programming the LDAP server.

- For details about specifying the search conditions, see Specifying the LDAP Address Search Conditions.

- For details about [Scanning Mode], see Scanner Settings.

- To configure advanced scan settings, see Specifying the Scan Settings.