ContentsPreviousNext
Settings

# Moving over a Long Distance

If you intend to move the machine over a long distance, you must pack it well. Empty all the paper trays, but do not remove the print cartridge. Take care not to tip or tilt the machine during transit.

- Do not remove the print cartridge when moving the machine.

Be sure to check the following points:

- The power switch is turned off.

- The power cord is unplugged from the wall outlet.

- All other cables are unplugged from the machine.

- All paper trays are empty.

If tray 2 is installed, remove it.

Return the scanning unit inside the machine to its original position using [Scanner Carriage] under [System Settings].

- Toner might spill inside the machine if the machine is not kept level during transit.

- For more information about moving the machine, contact your sales or service representative.

- For details about [Scanner Carriage], see System Settings.