ContentsPreviousNext
Settings

# Encryption Key Exchange Settings Configuration Flow

This section explains the procedure for specifying encryption key exchange settings.

Machine | PC
--- | ---
1. Set the IPsec settings on Web Image Monitor. | 1. Set the same IPsec settings as the machine on PC.
2. Enable IPsec settings. | 2. Enable IPsec settings.
3. Confirm IPsec transmission.

- After configuring IPsec, you can use "ping" command to check if the connection is established correctly. Because the response is slow during initial key exchange, it may take some time to confirm that transmission has been established.

- If you cannot access Web Image Monitor due to IPsec configuration problems, disable IPsec on the control panel, and then access Web Image Monitor.

- For details about disabling IPsec using the control panel, see Enabling and Disabling IPsec Using the Control Panel.