ContentsPreviousNext
Settings

# Configuring the POP3 Settings

Click the [POP3] tab on the network settings page to configure the POP3 settings.

POP3 Settings
Item | Description
--- | ---
POP3 Server | Enter the IP address or host name of the POP3 server for e-mail reception. The POP3 server specified here will be used for [POP before SMTP]. Can contain up to 64 characters.
User Account | Enter the user name for logging in to the POP3 server. Can contain up to 32 characters. If an e-mail address is entered here, the address will be used as the e-mail address for receiving Internet Faxes.
User Password | Enter the password for logging in to the POP3 server. Can contain up to 32 characters.
Authentication | Select an authentication method from the following: [None]: Password will not be encrypted. [APOP Authentication]: Password will be encrypted. [Auto]: Password will be encrypted or not encrypted according to the POP3 server’s settings.