ContentsPreviousNext
Settings

# Copier Function Specifications

Maximum resolution (scanning and printing)

- Exposure glass

  Scanning: 600 × 600 dpi

  Printing: 600 × 600 dpi

- ARDF/ADF

  Scanning: 600 × 300 dpi

  Printing: 600 × 600 dpi

Gradation

Scanning: 256 levels (1 dot)

Printing: Two-value (1 dot)

First copy speed (A4/Letter, at 25 °C, 77 °F)

12 seconds or less

Multiple copy speed

28 pages per minute

Reproduction ratio

- Fixed ratio: 50%, 71%, 82%, 93%, 122%, 141%, 200%, 400%

  Zoom ratio: 25 to 400% (600 × 300 dpi, 600 × 600 dpi)

- Fixed ratio: 50%, 65%, 78%, 93%, 129%, 155%, 200%, 400%

  Zoom ratio: 25 to 400% (600 × 300 dpi, 600 × 600 dpi)

Copy quantity

99