ContentsPreviousNext
Settings

# Registering the Special Senders

This section describes how to register Special Senders.

A maximum of 30 Special Senders can be registered.

Start the Web browser, and access the machine by entering its IP address.

Click [Special Sender].

From the [Destination Type] list, select [Special Sender].

Select the Special Sender number from the list (1 to 30).

Enter the Special Sender’s fax number (up to 20 characters).

Enter the administrator password if required.

Click [Apply].

Close the Web browser.

- A fax number can contain 0 to 9, “”, and space.