ContentsPreviousNext
Settings

# Basic Operation in Printer Mode

The following procedure explains how to perform basic printing.

Open the printer properties dialog box in your document's application.

Set printing options as necessary, and then click [OK].

The printer properties dialog box closes.

Click [OK].

- If printing is restricted, you must enter a user code in the printer driver's properties before sending a print job to the machine.

- If LDAP authentication is specified, you must enable user authentication and enter a user name and password in the printer driver's properties before sending a print job to the machine.

- If tray 2 is installed and automatic tray selection is specified for the print job, you can select the tray the machine uses first in [Paper Tray Priority] under system settings.

- If a paper jam occurs, printing stops after the current page has been printed out. After the jammed paper is removed, printing restarts from the jammed page automatically.

- After printing on envelopes, make sure to pull up the levers for printing on envelopes back to their original positions. Leaving the levers lowered can cause print quality problems when printing on paper other than envelopes.

- For details about accessing the printer properties, see Accessing the Printer Properties from an Application.

- For details about entering a user code, see When Machine Functions are Restricted.

- For details about enabling user authentication and entering a user name and password, see When LDAP Authentication is Specified.

- For details about [Paper Tray Priority], see System Settings.

- For details about how to remove the jammed paper, see Removing Printing Jams.

- For details about the levers for printing on envelopes, see Loading Envelopes.

Related topics

If a Paper Mismatch Occurs
Canceling a Print Job