ContentsPreviousNext
Settings

# Scanner Setting Parameters

This section describes the scanner setting parameters.

Scan Size

Specifies the scanning size according to the size of the original.

Default: [A4], [8 1/2 × 11]

- 8 1/2 × 14, 8 1/2 × 11, 8 1/2 × 5 1/2, 7 1/4 × 10 1/2, A4, B5, A5, Custom Size

Scanning Mode

Specifies the scanning mode using the control panel.

Default: [Colour]

- B&W

  The machine creates 1-bit black-and-white images. Images contain only black and white colors.

- Colour

  The machine creates 8-bit color images. Images are full color.

- Grey Scale

  The machine creates 8-bit black-and-white images. Images contain black and white, and intermediate gray colors.

Max. E-mail Size

Specifies the maximum size of a file that can be sent by e-mail.

Default: [1 MB]

- 1 MB

- 2 MB

- 3 MB

- 4 MB

- 5 MB

- No Limit

Density

Specifies the image density for scanning originals.

Default:

- (Lightest)

- (Darkest)

Resolution

Specifies the resolution for scanning the original.

Default: [300 × 300dpi]

- 100 × 100dpi

- 150 × 150dpi

- 200 × 200dpi

- 300 × 300dpi

- 400 × 400dpi

- 600 × 600dpi

Compression (Colour)

Specifies the color compression ratio for JPEG files. The lower the compression ratio, the higher the quality but greater the file size.

Default: [Medium]

- Low

- Medium

- High

Limitless Scan

Sets the machine to request next originals when scanning with the exposure glass.

Default: [Off]

- On

- Off

File Type

Specifies whether to create a multi-page file containing all pages or separate single-page files when scanning multiple pages.

Note that a scanned file can contain multiple pages only when the file format is PDF or TIFF. If the file format is JPEG, a single-page file is created for each scanned page.

Default: [Multi-page]

- Multi-page

- Single Page

Original

Sets the machine to scan both sides of original automatically when using the ARDF.

When using this function, specify the page and binding orientations according to those of the originals.

This setting appears only for the Type 2 model.

Default: [1 Sided]

- 1 Sided

- 2 Sided Portrait: T to T

- 2 Sided Portrait: T to B

- 2 Sided Landscape: T to T

- 2 Sided Landscape: T to B