ContentsPreviousNext
Settings

# Copy Setting Parameters

This section describes the copy setting parameters.

Select Paper

Specifies the paper size used for printing copies.

When a tray is selected, the machine prints from that tray only.

When a paper size is selected, the machine checks the trays for the paper of the specified size in the order of priority as set in [Paper Tray Priority] under system settings.

If multiple trays contain valid paper, the first tray the machine finds will be used for printing; when that tray runs out of paper, the machine automatically switches to the next tray to continue printing.

[Tray 2] appears only when tray 2 is installed.

Default: [Tray 1]

- Tray 1

- Tray 2

- Bypass Tray

- A4

- 8 1/2 × 11

Sort

Configures the machine to sort the output pages into sets when making multiple copies of a multi-page document (P1, P2, P1, P2...).

Default: [Off]

- On

- Off

Original Type

Specifies the content of originals, to optimize copy quality.

Default: [Mixed]

- Mixed

  Select this when the original contains both text and photographs or pictures.

- Text

  Select this when the original contains only text and no photographs or pictures.

- Photo

  Select this when the original contains photographs or pictures. Use this mode for the following types of original:

  - Photographs

  - Pages that are entirely or mainly photographs or pictures, such as magazine pages.

Density

Specifies the image density for photocopying.

Default:

- (Lightest)

- (Darkest)

Reduce/Enlarge

Specifies the percentage by which copies are enlarged or reduced. Also, ID card copying can be specified.

Default: [100%]

- 50%

- 65% ( model only)

- 71% ( model only)

- 78% ( model only)

- 82% ( model only)

- 93%

- 100%

- 122% ( model only)

- 129% ( model only)

- 141% ( model only)

- 155% ( model only)

- 200%

- 400%

- ID Card Copy

  Sets the machine to copy the front and back sides of an ID card, or other small document, onto the front of a single sheet of paper.

  Note that enabling this setting automatically disables combined/2-sided copying.

- Zoom 25-400%

Duplex/Combine

Specifies combined/2-sided copying. Select a copy mode according to your original and how you want the copy outputs to appear. For more details, see Combining Pages and Making 2-sided Copies.

Note that enabling combined/2-sided copying automatically disables ID card copying.

Default: [Off]

- Off

- 1Sd 2Orig->Comb 2on1 1Sd

  Copy will be made on 1 side, on which 2 pages of 1-sided original will be printed.

  - Portrait

  - Landscape

- 1Sd 4Orig->Comb 4on1 1Sd

  Copy will be made on 1 side, on which 4 pages of 1-sided original will be printed.

  - Portrait: L to R

  - Portrait: T to B

  - Landscape: L to R

  - Landscape: T to B

- 1 Sided Orig->2 Sided Copy (Type 2 model only)

  Copy will be made on 2 sides, on each of which 1 page of 1-sided original will be printed.

  - Portrait: T to T

  - Portrait: T to B

  - Landscape: T to T

  - Landscape: T to B

- 1Sd 4Orig->Comb 2on1 2Sd (Type 2 model only)

  Copy will be made on 2 sides, on each of which 2 pages of 1-sided original will be printed.

  - Portrait: T to T

  - Portrait: T to B

  - Landscape: T to T

  - Landscape: T to B

- 1Sd8Orig->Comb 4on1 2Sd (Type 2 model only)

  Copy will be made on 2 sides, on each of which 4 pages of 1-sided original will be printed.

  - Portrait: L to R, T to T

  - Portrait: L to R, T to B

  - Portrait: T to B, T to T

  - Portrait: T to B, T to B

  - Landscape: L to R, T to T

  - Landscape: L to R, T to B

  - Landscape: T to B, T to T

  - Landscape: T to B, T to B

- 2Sd 1Orig->Comb 2on1 1Sd (Type 2 model only)

  Copy will be made on 1 side, on each of which 2 pages of 2-sided original will be printed.

  - Portrait: T to T

  - Portrait: T to B

  - Landscape: T to T

  - Landscape: T to B

- 2Sd 2Orig->Comb 4on1 1Sd (Type 2 model only)

  Copy will be made on 1 side, on each of which 4 pages of 2-sided original will be printed.

  - Portrait: L to R, T to T

  - Portrait: L to R, T to B

  - Portrait: T to B, T to T

  - Portrait: T to B, T to B

  - Landscape: L to R, T to T

  - Landscape: L to R, T to B

  - Landscape: T to B, T to T

  - Landscape: T to B, T to B

- 2 Sided Orig->2 Sided Copy (Type 2 model only)

  Copy will be made on 2 sides, on each of which 2 pages of 2-sided original will be printed.

- 2Sd 2Orig->Comb 2on1 2Sd (Type 2 model only)

  Copy will be made on 2 sides, on each of which 2 pages of 2-sided original will be printed.

  - Portrait: T to T

  - Portrait: T to B

  - Landscape: T to T

  - Landscape: T to B

- 2Sd 4Orig->Comb 4on1 2Sd (Type 2 model only)

  Copy will be made on 2 sides, on each of which 4 pages of 2-sided original will be printed.

  - Portrait: L to R, T to T

  - Portrait: L to R, T to B

  - Portrait: T to B, T to T

  - Portrait: T to B, T to B

  - Landscape: L to R, T to T

  - Landscape: L to R, T to B

  - Landscape: T to B, T to T

  - Landscape: T to B, T to B

- Manual 2 Sided Scan Mode

  Enables the machine to scan both sides of an original and make a 2-sided copy using the exposure glass. When this setting is enabled, you will be asked to turn over the original on the exposure glass after scanning one side is complete.

  This setting is only available with the Type 2 model.