ContentsPreviousNext
Settings

# Making Enlarged or Reduced Copies

This section describes how to specify the reduction or enlargement ratio for the current job.

Scaling

There are two ways to set the scaling ratio: using a preset ratio or manually specifying a customized ratio.

- Preset ratio

  50%, 71%, 82%, 93%, 122%, 141%, 200%, 400%

  50%, 65%, 78%, 93%, 129%, 155%, 200%, 400%

- Custom ratio

  25% to 400% in 1% increments.

Use this procedure to specify the reduction or enlargement ratio for the current job.

Press the [Reduce/Enlarge] key.

Press [Reduce], [Enlarge], or [Zoom].

For [Reduce] or [Enlarge], press the [][][][] keys to select the desired ratio. For [Zoom], specify the desired ratio using the number keys.

Press the [OK] key.

- You can press the [Escape] key to exit to the previous level of the menu tree.

- You can change the machine's default [Reduce/Enlarge] setting to always make photocopies in the specified ratio.

- Temporary job settings are cleared in the following cases:

  - When no input is received for the period of time specified in [System Auto Reset Timer] while the initial screen is displayed.

  - When the [Clear/Stop] key is pressed while the initial screen is displayed.

  - When the machine's mode is changed.

  - When the power is turned off.

  - When the machine's default for the same setting is changed.

- For details about [Reduce/Enlarge], see Copy Settings.

- For details about [System Auto Reset Timer], see Administrator Settings.