ContentsPreviousNext
Settings

# Specifying a custom paper size

This section describes how to specify a custom paper size.

- Custom size paper cannot be loaded in tray 2.

- When you perform printing, make sure that the paper size specified with the printer driver matches the paper size specified with the control panel. If a paper size mismatch occurs, a message appears on the display. To ignore the error and print using mismatched paper, see "If a Paper Mismatch Occurs".

Press the [User Tools] key.

Press the [] [] keys to select [System Settings], and then press the [OK] key.

Press the [] [] keys to select [Tray Paper Settings], and then press the [OK] key.

Press the [] [] keys to select the paper size setting for the desired tray, and then press the [OK] key.

Press the [] [] [] [] keys to select [Custom Size], and then press the [OK] key.

Press the [] [] keys to select [mm] or [inch], and then press the [OK] key.

Enter the width using number keys, and then press the [OK] key.

To enter a decimal point, press [].

Enter the length using number keys, and then press the [OK] key.

To enter a decimal point, press [].

Press the [User Tools] key to return to the initial screen.

- You can press the [Escape] key to exit to the previous level of the menu tree.

- For details about printing using mismatched paper, see If a Paper Mismatch Occurs.