ContentsPreviousNext
Settings

# Configuring the Paper Settings

Click the [Tray Paper Settings] tab on the system settings page to configure the paper settings.

Tray 1
Item | Description
--- | ---
Paper Size | Select the paper size for tray 1 from the following: A4, B5 JIS, A5, B6 JIS, A6, 8 1/2 × 14, 8 1/2 × 11, 5 1/2 × 8 1/2, 7 1/4 × 10 1/2, 8 × 13, 8 1/2 × 13, 8 1/4 × 13, 16K, Custom Size
Paper Type | Select the paper type for tray 1 from the following: Thin Paper (52 to 64g/m2), Thick Paper 1 (100 to 130g/m2), Thick Paper 2 (131 to 162g/m2), Plain Paper, Recycled Paper, Color Paper, Preprinted Paper, Prepunched Paper, Letterhead, Bond Paper, Cardstock, Label Paper

Tray 2
Item | Description
--- | ---
Paper Size | Select the paper size for tray 2 from the following: A4, B5 JIS, A5, 8 1/2 × 14, 8 1/2 × 11, 5 1/2 × 8 1/2
Paper Type | Select the paper type for tray 2 from the following: Thin Paper (52 to 64g/m2), Thick Paper 1 (100 to 130g/m2), Plain Paper, Recycled Paper, Color Paper, Preprinted Paper, Prepunched Paper, Letterhead

Bypass Tray
Item | Description
--- | ---
Paper Size | Select the paper size for the bypass tray from the following: A4, B5 JIS, A5, B6 JIS, A6, 8 1/2 × 14, 8 1/2 × 11, 5 1/2 × 8 1/2, 7 1/4 × 10 1/2, 16K, 4 1/8 × 9 1/2, 3 7/8 × 7 1/2, C5 Env, C6 Env, DL Env, Custom Size
Paper Type | Select the paper type for the bypass tray from the following: Thin Paper (52 to 64g/m2), Thick Paper 1 (100 to 130g/m2), Thick Paper 2 (131 to 162g/m2), Plain Paper, Recycled Paper, Color Paper, Preprinted Paper, Prepunched Paper, Letterhead, Bond Paper, Cardstock, Label Paper, Envelope, OHP

Bypass Tray Setting Priority
Item | Description
--- | ---
Bypass Tray Setting Priority | Select how print jobs using the bypass tray are handled. System Settings The machine prints all print jobs according to the machine’s settings. An error will occur if the paper size/type settings of the machine and printer driver do not match. Any Size/Type The machine prints all print jobs according to the printer driver’s settings. Printing proceeds even if the paper size/type settings of the machine and printer driver do not match, but if the paper is too small for the print job, the printed image will be cropped. Any Custom Size/Type The machine prints custom size print jobs according to the printer driver’s settings and prints standard size print jobs according to the machine’s settings. For custom size print jobs, printing proceeds even if the paper size/type settings of the machine and printer driver do not match, but if the paper is too small for the print job, the printed image will be cropped. For standard size print jobs, an error will occur if the paper size/type settings of the machine and printer driver do not match.

- The information about tray 2 appears only when it is installed.