ContentsPreviousNext
Settings

# Turning the Power on

This section describes how to turn on the machine.

| Do not use any power sources other than those that match the specifications shown in this manual. Doing so could result in fire or electric shock.

| Do not use any frequencies other than those that match the specifications shown. Doing so could result in fire or electric shock.

| Do not use multi-socket adaptors. Doing so could result in fire or electric shock.

| Do not use extension cords. Doing so could result in fire or electric shock.

| Do not use power cords that are damaged, broken, or modified. Also, do not use power cords that have been trapped under heavy objects, pulled hard, or bent severely. Doing so could result in fire or electric shock.

| Touching the prongs of the power cable's plug with anything metallic constitutes a fire and electric shock hazard.

| The supplied power cord is for use with this machine only. Do not use it with other appliances. Doing so could result in fire or electric shock.

| It is dangerous to handle the power cord plug with wet hands. Doing so could result in electric shock.

| Be sure to push the plug of the power cord fully into the wall outlet. Partially inserted plugs create an unstable connection that can result in unsafe buildup of heat.

| If this machine is not going to be used for several days or longer at a time, disconnect its power cord from the wall outlet.

| When performing maintenance on the machine, always disconnect the power cord from the wall outlet.

- Make sure that the power cord is plugged securely into the wall outlet before turning the power on.

- Make sure that the power is off when plugging or unplugging the power cord.

- Do not turn off the power switch until initializing is completed. Doing so results in malfunction.

Plug in the power cord.

Insert the plug of the power cord into the wall socket securely.

Turn the power switch to ”On”.

The Power indicator lights up, and then the [Copy] key on the control panel lights up.

- Depending on the [Function Priority] setting under [Admin. Tools], the [Facsimile] or [Scanner] key may light up instead of the [Copy] key.

- The machine may make a noise while initializing. This noise does not indicate a malfunction.

- To turn off the power, turn the power switch to “ Off”.

- For details about [Function Priority], see Administrator Settings.