ContentsPreviousNext
Settings

# Placing Originals

This section describes the procedure for placing originals on the exposure glass and in the ARDF or ADF.

- Do not place originals before any correction fluid and toner has completely dried. Doing so may make marks on the exposure glass that will appear on copies.

- The original in the ARDF or ADF takes precedence over the original on the exposure glass if you place originals both in the ARDF/ADF and on the exposure glass.

- Because colors made by marker or highlighter pen on originals are difficult to reproduce, they might not appear on copies.

Related topics

Placing originals on the exposure glass
Placing originals in the ARDF (Type 2 model)
Placing originals in the ADF (Type 1 model)