Hands-Free Smart-Phone Bluetooth Connection:

2016 Japanese (Kanji) Leaf - Hands-Free Smart-Phone Connection. Within this touch-panel translation 'guide' we need a step-by-step instruction for making a smart-phone blue-tooth connection to the hands-free system provided within the leaf.
Can you please produce this instruction including the touch-panel button sequence. Perhaps a flow-chart with the Kanji legend on the touch-screen would provide the best guide?
ChatGPT – 1st Response:
Alan, this is a very worthwhile addition to the 2016 Japanese-market Nissan Leaf G-Trim Touch-Panel English Guide you have been developing. The hands-free phone pairing procedure is one of the areas where the Japanese Kanji interface creates the greatest difficulty for an English-speaking owner.
For your guide, I suggest presenting it as a simple flow-chart first, followed by a button-by-button explanation. The exact Kanji wording can vary slightly depending on the Japanese navigation/audio unit fitted, but the sequence below matches the common Nissan Connect / CARWINGS touch-screen systems fitted to the ZE0/AZE0 Leaf generation.
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2016 Nissan Leaf (AZE0)
Bluetooth Hands-Free Phone Pairing Guide - Japanese Touch Panel → English Translation

Quick Flow Chart
START
│
▼
Press AUDIO button
(オーディオ)
│
▼
Press SETTING button
(設定)
│
▼
Select Bluetooth
(Bluetooth設定)
│
▼
Select Register Phone
(携帯電話登録)
│
▼
Touch "Add New"
(新規登録)
│
▼
Leaf displays:
"Waiting for Bluetooth connection"
│
▼
On Smartphone:
Settings
↓
Bluetooth ON
↓
Search Devices
↓
Select:
"NISSAN CONNECT"
or
"NISSAN"
│
▼
Confirm PIN code
(usually 0000 or displayed number)
│
▼
Pairing Complete
登録完了
│
▼
Enable:
Hands-Free Calling
Contacts Transfer (optional)
│
▼
FINISHED

Detailed Touch-Screen Button Sequence
Step 1 — Turn Vehicle ON
1. Press brake pedal.
2. Press POWER button.
3. Allow the centre display to start.

Step 2 — Open Audio Menu
Touch:
オーディオ
AUDIO
Meaning:
Audio system menu

Step 3 — Open Settings
Touch:
設定
SETTING
Meaning:
System settings

Step 4 — Bluetooth Menu
Look for:
Bluetooth設定
English:
Bluetooth Settings
Possible alternative:
電話設定
English:
Phone Settings

Step 5 — Register a New Phone
Touch:
携帯電話登録
English:
Register Mobile Phone
or:
新規登録
English:
New Registration / Add Device

Step 6 — Vehicle Waiting Mode
The Leaf screen should show a message similar to:
Bluetooth接続待機中
Meaning:
Waiting for Bluetooth connection
The vehicle is now ready to be discovered.

Step 7 — Smartphone Procedure
On the smartphone:
SETTINGS
↓
Bluetooth
↓
Turn ON
↓
Search for devices
The phone should find something like:
NISSAN CONNECT
or
NISSAN
Select it.

Step 8 — Confirm Pairing Code
The Leaf and phone should display a PIN.
Common Nissan PIN:
0000
or
1234
or a generated number.
Confirm:
Phone:
PAIR
Leaf: はい
YES

Step 9 — Phone Functions
After pairing, the Leaf may ask:
Transfer phone book?
Japanese:
電話帳転送
Meaning:
Transfer Contacts
Recommended:
はい
YES

Automatic Connection
Enable:
自動接続
Meaning:
Automatic Connection
Recommended:
ON

Kanji Quick Reference Table
	Japanese
	English Meaning

	設定
	Settings

	オーディオ
	Audio

	電話
	Phone

	Bluetooth
	Bluetooth

	Bluetooth設定
	Bluetooth Settings

	携帯電話
	Mobile Phone

	登録
	Register

	新規登録
	New Registration

	削除
	Delete

	接続
	Connect

	切断
	Disconnect

	電話帳
	Phone Book

	転送
	Transfer

	はい
	Yes

	いいえ
	No

	戻る
	Back



Steering Wheel Operation After Pairing
Once connected:
Receive call
Press:
☎ button
(on steering wheel)

End call
Press:
☎ button again

Voice operation
Press:
Voice button
(if fitted)

Recommended Addition to Your Leaf Guide
For the A4 beginner guide, I would place this as:
Chapter 4 — Connecting Your Smartphone
with:
Page 1:
Large flow-chart above.
Page 2:
Actual screen sequence:
Audio
 ↓
Setting
 ↓
Bluetooth
 ↓
Register Phone
 ↓
Pair
Page 3:
Kanji reference card.
This will complement the earlier chapters covering:
1. Driver's view
2. Three display panels
3. Steering-wheel buttons
4. Touch-screen navigation
5. LeafSpy

One important note: because your Leaf is a 2016 Japanese domestic AZE0 G-Trim, there is a possibility that the fitted Nissan Connect unit is one of several Japanese variants (with CARWINGS, TV tuner, or different firmware). If you can later provide a clear photograph of the main Audio/Navigation screen showing the bottom-row buttons, I can produce a screen-by-screen facsimile guide matching your exact Kanji menus rather than the generic AZE0 sequence above.
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